START-INFO-DIR-ENTRY
* mjpegtools: (mjpeg-howto).       command line tools for MPEG audio and video.
END-INFO-DIR-ENTRY

\input texinfo


File: mjpeg-howto.info,  Node: Top,  Next: Introduction,  Up: (dir)

MJPEG HOWTO - An introduction to the MJPEG-tools
************************************************

     Praschinger Bernhard
     v1.50

   MJPEG capture/editting/replay and MPEG encoding toolset description

* Menu:

* Introduction::
* Unsorted list of useful Hints::
* Recording videos::
* Creating videos from other sources::
* Checking if recording was successful::
* Edit the video::
* Converting the stream to MPEG or DIVx videos::
* Optimizing the stream::
* Transcoding of existing MPEG-2::
* Trading Quality/Speed::
* SMP and distributed Encoding::
* Interoperability::


File: mjpeg-howto.info,  Node: Introduction,  Next: Unsorted list of useful Hints,  Prev: Top,  Up: Top

1 Introduction
**************

I wrote this things down, because I had many sheets with notes on them.
This should be some kind of summary of collected knowledge of this
sheets.  Andrew Stevens helped with encoding and VCD knowledge and
hints.

   The mjpegtools are a set of programs that can do recording,
playback, editing and eventual MPEG compression of audio and video
under Linux.

   Although primarily intended for use with capture / playback boards
based on the Zoran ZR36067 MJPEG codec chip, the mjpegtools can easily
be used to process and compress MJPEG video streams captured using
xawtv using simple frame-buffer devices.

   The HOWTO for the tools intended to give an an introduction to the
MJPEG-tools and the creation of MPEG 1/2 videos. VCD and SVCD, and the
transcoding of existing mpeg streams.

   For more information about the programs read the corresponding
man-page.

   Achtung es gibt auch eine deutsche Version bei:
http://sourceforge.net/projects/mjpeg

   There is also a manpage of this text, you can read it with "man
mjpegtools" if installed.  We also have a info version you should be
able to read it with info

   The text version of this text is available via cvs, you should get
it with a tarball or the precompiled package (RPM and deb).

   In the following picture you see the typical workflow when you
record a video.  Cut it afterwards and encode it. In the picture you
also see the connections to other programs. These parts are in grey,
the parts in blue can be done with the mjpegtools.

                        Video encoding workflow


File: mjpeg-howto.info,  Node: Unsorted list of useful Hints,  Next: Recording videos,  Prev: Introduction,  Up: Top

2 Unsorted list of useful Hints
*******************************

You have to compile and install the mjpeg_play package, for this read
the README & REQUIRED_SOFTWARE & INSTALL.  If you do not want to
compile it, you can download the mjpeg .RPM or .DEB package at
Sourceforge.

   There is a script in the scripts/ directory. This script is
something that show's you a way how it can be done. It also creates
(under certain circumstances) videos that look quite good. Better
videos you only get by tuning the parameters yourself.

   If you use a Linux kernel from the 2.4 series, you will usually have
to load the drivers for the Buz or DC10 or LML33 cards.So you have to
run the update script providing as option the name of your card you
have. The script is usually in /usr/src/driver-zoran/.  The zoran
kernel driver below the kernel 2.4.4 do not work.  You have to use the
driver available from: http://mjpeg.sourceforge.net/driver-zoran

   In the 2.6. Linux kernel is the driver for the zoran cards included,
you just need to make soure that it is loaded correct.

   The driver for the Matrox Marvel card also works, more information
about it: http://marvel.sourceforge.net

   If you compile the tools on a P6 based computer (PPro, P-II, P-III,
P-4, Athlon,Duron) then never try to let them run on a P5 based computer
(Pentium, Pentium-MMX, K6, K6-x, Cyrix, Via, Winchip). You'll get a
"illegal instruction" and the program won't work.

   If lav2yuv dumps core then one possible cause is no dv support was
included. To enable it make sure that libdv is installed on the system.
This will be necessary if you are using a digital camera (or analog to
DV converter such as the Canopus ADVC100) and converting the dv avi
format into the MPEG format.

   Start xawtv to see if you get an picture. If you want to use
HW-playback of the recorded streams you have to start xawtv (any TV
application works) once to get the streams played back. You should also
check the settings of your mixer in the sound card.

   If you compile the tools on a platform other than Linux not all tools
will work.   Mjpegtools on a OS/X system for example will not have V4L
(video4linux) capability.

   Never try to stop or start the TV application when lavrec runs. If
you start or stop the TV application lavrec will stop recording, or
your computer could get "frozen". This is a problem of v4l
(video4linux).

   This problem is solved with v4l2. If you use v4l2 you can record the
video and stop and start the tv application whenever you want.  But
v4l2 is currently (7. Jan. 2003) only supported for the zoran based
cards (BUZ, DC10, DC10+, LML33) if you use the CVS driver from
mjpeg.sf.net tagged with ZORAN_VIDEODEV_2.  And this driver only works
with the 2.4.20 kernel and the 2.5.* development kernel.

   One last thing about the data you get before we start:

   Audio: ( Samplerate * Channels * Bitsize ) / (8 * 1024) CD
Quality:(44100 Samples/sec * 2 Chanels * 16 Bit) / (8 * 1024)=172,2
kB/sec

   The 8 * 1024 convert the value from bit/sec to kByte/sec

   Video: (width * height * framerate * quality ) / (200 * 1024) PAL
HALF Size : (352 * 288 * 25 * 80) / (200 * 1024) = 990 kB/sec PAL FULL
size : (720 * 576 * 25 * 80) / (200 * 1024) = 4050 kB/sec NTSC HALF
size: (352 * 240 * 30 * 80) / (200 * 1024) = 990 kB/sec NTSC FULL size:
(720 * 480 * 30 * 80) / (200 * 1024) = 4050 kB/sec

   The 1024 converts the Bytes to kBytes. Not every card can record the
size mentioned. The Buz and Marvel G400 for example can only record a
size of 720x576 when using -d 1, the DC10 records a size of 384x288
when using -d 2.

   When you add audio and video datarate this is what your hard disk
has to be able to write constantly streaming, else you will have lost
frames.

   If you want to play with the `-mjpeg-buffer-size'. Remember the value
should be at least big enough that one frame fits in it. The size of
one frame is: (width * height * quality ) / (200 * 1024) = kB If the
buffer is too small the rate calculation doesn't match any more and
buffer overflows can happen. The maximum value is 512kB.

   How video works and the difference between the video types is
explained here: http://www.mir.com/DMG/

   There you also find how to create MPEG Still Images for VCD/SVCD.

   A good description of DV (Digital Video) can be found here:
http://www.uwasa.fi/~f76998/video/conversion/

* Menu:

* Some books we found usefull::


File: mjpeg-howto.info,  Node: Some books we found usefull,  Up: Unsorted list of useful Hints

2.1 Some books we found usefull
===============================

written in English:
   * Digital Video and HDTV by Charles Poyton (ISBN 1-55860-792-7)

   * Digital Video Compression by Peter Symes (ISBN 0-07-142487-3)

   * Video Demystified by Keith Jack (ISBN 1-878707-56-6)

   written in German:
   * Fernsehtechnik von Rudolf Maeusl (ISBN 3-7785-2374-0)

   * Professionelle Videotechnik - analoge und digitale Grundlagen von
     U. Schmidt (ISBN 3-540-43974-9)

   * Digitale Film- und Videotechnik von U. Schmidt (ISBN 3-446-21827-0)

   If you know some other really good book about that, write us!


File: mjpeg-howto.info,  Node: Recording videos,  Next: Creating videos from other sources,  Prev: Unsorted list of useful Hints,  Up: Top

3 Recording videos
******************

* Menu:

* lavrec examples::
* Other recording hints::
* Some information about the typical lavrec output while recording::
* Notes about "interlace field order - what can go wrong and how to fix it"::


File: mjpeg-howto.info,  Node: lavrec examples,  Next: Other recording hints,  Up: Recording videos

3.1 lavrec examples
===================

Recording with lavrec look's like this:

   `> lavrec -f a -i P -d 2 record.avi'

`'
     Should start recording now,

`-f a'
     use AVI as output format,

`-i P'
     use as input source the SVHS-In with PAL format,

`-d 2'
     the size of the pictures are half size (352x288)

`record.avi'
     name of the created file.


   Recording is finished by pressing Ctrl-C (on German Keyboards:
Strg-C).  Sometimes using `-f A' instead of `-f a' might be necessary

   Other example:

   `> lavrec -f q -i n -d 1 -q 80 -s -l 80 -R l -U record.avi '

`'
     Should start recording now,

`-f q'
     use Quicktime as output format,

`-i n'
     use Composite-In with NTSC format,

`-d 1'
     record pictures with full size (640x480)

`-q 80'
     set the quality to 80% of the captured image

`-s'
     use stereo mode (default mono)

`-l 80'
     set the recording level to 80% of the max during recording

`-R l'
     set the recording source to Line-In

`-U'
     With this lavrec uses the read instead of mmap for recording this
     is needed if your sound card does not support the mmap for
     recording.


   Setting the mixer does not work with every sound card.  If you
record with 2 different settings and both recordings are equally loud
you should setup the mixer with a mixer program.  After that you should
use the `-l -1' option when you record using lavrec

   The size of the image depends on the card you use.  At full size (-d
1) you get these image sizes: BUZ and LML33: 720x576, the DC10 and
DC30: 768x576

   Other example:

   `> lavrec -w -f a -i S -d 2 -l -1 record%02d.avi'

`'
     Should start recording,

`-w'
     Waits for user confirmation to start (press enter)

`-f a'
     use AVI as output format,

`-i S'
     use SECAM SVHS-Input (SECAM Composite recording is also possible:
     -i s)

`-d 2'
     the size of the pictures are half size

`-l -1'
     do not touch the mixer settings

`record%02d.avi'
     Here lavrec creates the first file named record00.avi after the
     file has reached a size of 1.6GB (after about 20 Minutes
     recording) it starts a new sequence named record01.avi and so on
     till the recording is stopped or the disk is full. With the
     release of the 1.9.0 Version, the mjpegtools are able to handle
     AVI files larger than 2GB. So that option is not needed any more
     if you want to record more data that fits into a 2GB file.


   Other example:

   `> lavrec -f a -i t -q 80 -d 2 -C europe-west:SE20 test.avi'

`'
     Should start recording now,

`-f a'
     use AVI as output format,

`-i t'
     use tuner input,

`-q 80'
     set the quality to 80% of the captured image

`-d 2'
     the size of the pictures are half size (352x288)

`-C'
     choose TV channels, and the corresponding -it and -iT (video
     source: TV tuner) can currently be used on the Marvel G200/G400
     and the Matrox Millenium G200/G400 with Rainbow Runner extension
     (BTTV-Support is under construction). For more information on how
     to make the TV tuner parts of these cards work, see the
     Marvel/Linux project on: http://marvel.sourceforge.net


   Last example:

   `> lavrec -f a -i p -g 352x288 -q 80 -s -l 70 -R l -software-encoding
test03.avi'

   The two new options are `-g 352x288', which sets the size of the
video to be recorded when using `-software-encoding', this enables the
software encoding of the recorded images. With this option you can also
record from a bttv based card. The processor load is high. This option
only works for generic video4linux cards (such as the brooktree-848/878
based cards), it doesn't work for zoran-based cards.


File: mjpeg-howto.info,  Node: Other recording hints,  Next: Some information about the typical lavrec output while recording,  Prev: lavrec examples,  Up: Recording videos

3.2 Other recording hints
=========================

All lavtools accept a file description like file*.avi, so you do not
have to name each file, but that would also be a posibillity to do.

   Note: More options are described in the man-page, but with this you
should be able to get started.

   Here are some hints for sensible settings. Turn the quality to 80%
or more for -d 2 capture. At full resolution as low as 40% seems to be
visually "perfect". -d 2 is already better than VHS video (a *lot*!).
For a Marvel you should not set the quality higher than 50 when you
record at full size (-d 1). If you use higher settings (-q 60) it is
more likely that you will encounter problems. Higher settings will
result in framedrops.  If you're aiming to create VCD's then there is
little to be gained recording at full resolution as you need to reduce
to -d 2 resolution later anyway.

   you can record at other sizes than the obvious -d 1/2/4. You can use
combinations where you use halve horizontal size and full vertical
size: -d 21.  This would record for NTSC at a size of 352x480. This
helps if you want to create SVCDs, scaling the 352 Pixles put to 480 is
not that visible for the eye as if you would use the other combination
-d 12.  Where you have the full horzontal resolution and half vertical
this Version will have a size of 720x288 for NTSC


File: mjpeg-howto.info,  Node: Some information about the typical lavrec output while recording,  Next: Notes about "interlace field order - what can go wrong and how to fix it",  Prev: Other recording hints,  Up: Recording videos

3.3 Some information about the typical lavrec output while recording
====================================================================

0.06.14:22 int: 00040 lst:0 ins:0 del:0 ae:0 td1=0.014 td2=0.029

   The first part shows the time lavrec is recording.  `int:' the
interval between two frames. `lst:' the number of lost frames. `ins and
del:' are the number of frames inserted and deleted for sync
correction. `ae:' number of audio errors.  `td1 and td2' are the
audio/video time-difference.

   *  `[int] frame interval' should be around 33 (NTSC) or 40
     (PAL/SECAM). If it is very different, you'll likely get a bad
     recording and/or many lost frames

   *  `[lst] lost frames' are bad and mean that something is not working
     very well during recording (too slow HD, too high CPU usage, ...)
     Try recording with a greater decimation and possibly a lower
     quality.

   *  `[ins, del] inserted OR deleted frames' of them are normal ->
     sync. If you have many lost AND inserted frames, you're asking too
     much of your machine.  Use less demanding options or try a
     different sound card.

   *  `[ae] audio errors' are never good. Should be 0

   *  `[td1, td2] time difference'is always floating around 0, unless
     sync correction is disabled (-synchronization!=2, 2 is default).


File: mjpeg-howto.info,  Node: Notes about "interlace field order - what can go wrong and how to fix it",  Prev: Some information about the typical lavrec output while recording,  Up: Recording videos

3.4 Notes about "interlace field order - what can go wrong and how to fix it"
=============================================================================

Firstly, what does it mean for interlace field order to be wrong?

   The whole mjpegtools image processing chain is frame-oriented. Since
it is video material that is captured each frame comprised a top field
(the 0th, 2nd, 4th and so lines) and a bottom field (the 1st, 3rd, 5th
and so on lines).

* Menu:

* There are three bad things that can happen with fields::
* How can I recognize if I have one of these Problems ?::
* How can you fix it?::
* Hey what about NTSC movies ?::


File: mjpeg-howto.info,  Node: There are three bad things that can happen with fields,  Next: How can I recognize if I have one of these Problems ?,  Up: Notes about "interlace field order - what can go wrong and how to fix it"

3.4.1 There are three bad things that can happen with fields
------------------------------------------------------------

  1.  This is really only an issue for movies in PAL video where each
     film frame is sent as a pair of fields. These can be sent top or
     bottom field first and sadly it's not always the same, though
     bottom-first appears to be usual. If you capture with the wrong
     field order (you start capturing each frame with a bottom rather
     than a top or vice versa) the frames of the movie get split
     *between* frames in the stream. Played back on a TV where each
     field is displayed on its own this is harmless. The sequence of
     fields played back is exactly the same as the sequence of fields
     broadcast. Unfortunately, playing back on a Computer monitor where
     both fields of a frame appear at once it looks *terrible* because
     each frame is effectively mixing two moments in time 1/25sec
     apparent.

  2.  The two fields can simply be swapped somehow so that top gets
     treat as bottom and bottom treat as top. Juddering and "slicing"
     is the result. This occasionally seems to happen due to hardware
     glitches in the capture card.

  3.  Somewhere in capturing/processing the *order* in time of the two
     fields in each frame can get mislabeled somehow. This is not good
     as it means that when playback eventually takes place a field
     containing an image sampled earlier in time comes after an image
     sampled later.  Weird "juddering" effects are the results.


File: mjpeg-howto.info,  Node: How can I recognize if I have one of these Problems ?,  Next: How can you fix it?,  Prev: There are three bad things that can happen with fields,  Up: Notes about "interlace field order - what can go wrong and how to fix it"

3.4.2 How can I recognize if I have one of these Problems ?
-----------------------------------------------------------

  1. This can be hard to spot. If you have mysteriously flickery
     pictures during playback try encoding a snippet with the reverse
     field-order forced (see below). If things improve drastically you
     know what the problem was and what the solution is!

  2. The two fields can simply be swapped somehow so that top gets treat
     as bottom and bottom treat as top. Juddering and "slicing" is the
     result. This occasionally seems to happen due to hardware glitches
     in the capture card. That problem lookes like that:

                            Interlacing problem

  3. Somewhere in capturing/processing the *order* in time of the two
     fields in each frame can get mislabeled somehow. This is not good
     as it means that when playback eventually takes place a field
     containing an image sampled earlier in time comes after an image
     sampled later. Weird "juddering" effects are the result.

   If you use glav or lavplay be sure that you also use the
`-F/-flicker' option. This disables some things that make the picture
look better.

   If you want to look at the video you can also use yuvplay:

   `> lav2yuv | ... | yuvplay'

   If there is a field order problem you should see it with yuvplay.


File: mjpeg-howto.info,  Node: How can you fix it?,  Next: Hey what about NTSC movies ?,  Prev: How can I recognize if I have one of these Problems ?,  Up: Notes about "interlace field order - what can go wrong and how to fix it"

3.4.3 How can you fix it?
-------------------------

  1. To fix this one the fields need to be "shifted" through the
     frames. Use yuvcorrect's `-T BOTT_FORWARD/TOP_FORWARD' to shift
     the way fields are allocated to frames. You can find out the
     current field order for an MJPEG file by looking at the first few
     lines of debug output from: `> lav2yuv -v 2 the_mjpeg_file >
     /dev/null' Or re-record exchanging `-f a' for `-F A' or vice-versa.

  2. This isn't too bad either. Use a tool that simply swaps the top
     and bottom fields a second time. yuvcorrect can do this use the
     `-T LINE_SWITCH'.

  3. Is easy to fix. Either tell a tool someplace to relabel the fields
     or simply tell the player to play back in swapped order (the
     latter can be done "indirectly" by telling mpeg2enc when encoding
     to `reverse the flag (-z b|t)' that tells the decoder which field
     order to use.

   `In order to determine exactly what type of interlacing problem you
have, you need to extract some frames from the recorded stream and take
a look at them:'

   > mkdir pnm > lav2yuv -f 40 video.avi | y4mtoppm | pnmsplit -
pnm/image%d.pnm > rm pnm/image?.pnm > cd pnm > xv

   First we create a directory where we store the images. The lav2yuv
-f 40 writes only the first 40 frames to stdout. The mjpegtools
y4mtoppm converts the frames to pnm images and the pnmsplit splits the
picture into two frames in the picture to two single pictures. Then we
remove the first 10 images because pnmsplit does not support the %0xd
numbering. Without a leading zero in the number, the files will be
sorted in the wrong order, leading to confusing playback.

   Use your favorite graphic program (xv for example) to view the
pictures. As each picture only contain one field out of two they will
appear scaled vertically. If you look at the pictures you should see
the movie slowly advancing.

   If you have a film you should always see 2 pictures that are nearly
the same (because the film frame is split into two field for
broadcasting) after each other.  You can observe this easily if you
have comb effects when you pause the film because both fields will be
displayed at the same time. The two pictures that belong together
should have an even number and the following odd number. So if you take
a look on pictures: 4 and 5 are nearly identical, 5 and 6 differ (have
movement), 6 and 7 identical, 7 and 8 differ , ....

   To fix this problem you have to use yuvcorrect's `-T BOTT_FORWARD or
TOP_FORWARD'. You can also have the problem that the field order
(top/bottom) is still wrong. You may have to use yuvcorrect a second
time with `-M LINE_SWITCH', or use the mpeg2enc `-z (b|t)' option.

   To see if you guessed correctly, extract the frames again,
reordering them using yuvcorrect:

   `> lav2yuv -f 40 video.avi | yuvcorrect -T OPTION | y4mtoppm |
pnmsplit - pnm/image%d.pnm '

   Where "OPTION" is what you think it will corrects the problem.  This
is for material converted from film. Material produced directly for TV
is addressed below.


File: mjpeg-howto.info,  Node: Hey what about NTSC movies ?,  Prev: How can you fix it?,  Up: Notes about "interlace field order - what can go wrong and how to fix it"

3.4.4 Hey what about NTSC movies ?
----------------------------------

Movies are broadcast in NTSC using "3:2" pulldown which means that half
the capture frames contain fields from 1 movie frame and half fields
from 2 frames. To undo this effect for efficient MPEG encoding you need
to use yuvkineco.

   If you have an interlaced source like a TV camera you have a frame
consists of two fields that are recorded at different points in time
and shown after each other. Spotting the problem here is harder. You
need to find something moving horizontally from the left to the right.
When you extract the fields, the thing should move in small steps from
the left to the right, not one large step forward, small step back,
large forward, small back......  You have to use the same options
mentioned aboth to correct the problem.

   Do not expect that the field order is always the same (top- or
bottom-first) It may change between the channels, between the films,
and it may even change within a film. If it changes constant you may
have to encode with the mpeg2enc -I 1 or even -I 2.

   You can only have this problems if you record at full size !!!


File: mjpeg-howto.info,  Node: Creating videos from other sources,  Next: Checking if recording was successful,  Prev: Recording videos,  Up: Top

4 Creating videos from other sources
************************************

Here are some hints and descriptions of how to create the videos from
other sources like images and other video types.

   You might also be interested in taking a look at the `Transcoding of
existing MPEG-2' section.

* Menu:

* Creating videos from images::
* Decoding streams with mplayer::
* Decoding MPEG2 streams with mpeg2dec::
* Other things to know::


File: mjpeg-howto.info,  Node: Creating videos from images,  Next: Decoding streams with mplayer,  Up: Creating videos from other sources

4.1 Creating videos from images
===============================

You can use jpeg2yuv to create a yuv stream from separate JPEG images.
This stream is sent to stdout, so that it can either be saved into a
file, encoded directly to a mpeg video using mpeg2enc or used for
anything else.

   Saving an yuv stream can be done like this:

   `> jpeg2yuv -f 25 -I p -j image%05d.jpg > result.yuv'

   Creates the file result.yuv containing the yuv video data with 25
FPS. The -f option is used to set the frame rate. Note that
image%05d.jpg means that the jpeg files are named image00000.jpg,
image00001.jpg and so on. (05 means five digits, 04 means four digits,
etc.) The -I p is needed for specifing the interlacing. You have to
check which type you have.  If you don't have interlacing just choose p
for progressive

   If you want to encode a mpeg video directly from jpeg images without
saving a separate video file type:

   `> jpeg2yuv -f 25 -I p -j image%05d.jpg | mpeg2enc -o mpegfile.m1v'

   Does the same as above but saves a mpeg video rather than a yuv
video. See mpeg2enc section for details on how to use mpeg2enc.

   You can also use yuvscaler between jpeg2yuv and mpeg2enc. If you
want to create a SVCD from your source images:

   `> jpeg2yuv -f 25 -I p -j image%05d.jpg | yuvscaler -O SVCD |
mpeg2enc -f 4 -o video.m2v'

   You can use the -b option to set the number of the image to start
with. The number of images to be processed can be specified with the -n
number. For example, if your first image is image01.jpg rather than
image00.jpg, and you only want 60 images to be processed type:

   `>jpeg2yuv -b 1 -f 25 -I p -n 60 -j image*.jpg | yuv2lav -o
stream_without_sound.avi'

   Adding the sound to the stream then:

   `> lavaddwav stream_without_sound.avi sound.wav
stream_with_sound.avi'

   For ppm input there is the ppmtoy4m util. There is a manpage for
ppmtoy4m that should be consulted for additional information.

   So to create a mpeg video try this:

   `>cat *.ppm | ppmtoy4m -o 75 -n 60 -F 25:1 | mpeg2enc -o output.m1v'

   Cat's each *.ppm file to ppmtoy4m. There the first 75 frames
(pictures) are ignored and next 60 are encoded by mpeg2enc to
output.m1v. You can run it without the -o and -n option. The -F
options sets the frame rate, default is NTSC (30000:1001), for PAL you
have to use -F 25:1.

   Other picture formats can also be used if there is a converter to
ppm.

   `>ls *.tga | xargs -n1 tgatoppm | ppmtoy4m | yuvplay'

   A list of filenames (ls *.tga) is given to xargs that executes the
tgatoppm with one (-n 1) argument per call, and feeds the output into
ppmtoy4m.  This time the video is only shown on the screen. The xargs
is only needed if the converter (tgatoppm), can only operate on a
single image at a time.

   If you want to use the ImageMagick 'convert' tool (a Swiss Army
Knife) try:

   `>convert *.gif ppm:- | ppmtoy4m | yuvplay'

   That means take all '.jpg' images in directory, convert to PPM
format, and pipe to stdout, then ppmtoy4m processes them ....


File: mjpeg-howto.info,  Node: Decoding streams with mplayer,  Next: Decoding MPEG2 streams with mpeg2dec,  Prev: Creating videos from images,  Up: Creating videos from other sources

4.2 Decoding streams with mplayer
=================================

Decoding the streams with mplayer is a nice way of bringing every video
that mplayer can play back to something you can edit or encode directly
to a mpeg video with the mjpegtools. This method has been tested with
mplayer 1.0rc2. And should work with modifications of the mplayer
commandline also with newer and older versions

   `>mkfifo stream.yuv'

   `>cat stream.yuv | yuv2lav -o mjpeg_wo.avi &'

   `>mplayer -nosound -noframedrop -vo yuv4mpeg anyfile.mpg'

   `>mplayer -vo null -ao pcm:file=anyfile.wav anyfile.mpg'

   Now you have for example a mjpeg encoded AVI without sound. The
sound will be in anyfile.wav. Now you can choose if you want to add the
sound to the AVI with `lavaddwav' and edit the file and encode it.

   You can also use instead of yuv2lav, mpeg2enc or any other tool from
the mjpeg tools so your command might also look like that:

   `> cat stream.yuv | yuvdenoise | yuvscaler -O SVCD | mpeg2enc -f 4
-o video_svcd.m2v'

   And cat the wav file into `mp2enc' to encode it to MP2 audio. The
`-vo yuv4mpeg' option works well with other input types mentioned in
the mplayer documentation.


File: mjpeg-howto.info,  Node: Decoding MPEG2 streams with mpeg2dec,  Next: Other things to know,  Prev: Decoding streams with mplayer,  Up: Creating videos from other sources

4.3 Decoding MPEG2 streams with mpeg2dec
========================================

You can decode mpeg2 streams with the patched mpeg2dec version which
creates yuv streams. You can pipe that into any other mjpegtools
program.  Or you use a mpeg2dec version directly from the libmpeg2
project and use the output mode pgmpipe. With the `pgmtoy4m' program
from the mjpegtools you can convert that pgm output back to yuv.

   If you ask yourself why there is a patched version and pgmtoy4m.
The answer is that the patch for yuv output was sent several times to
the libmpeg2 developers but was never included.  Now we have two ways
around that problem. Decoding looks like this:

   `> mpeg2dec -s -o pgmpipe ANYTS.VOB | pgmtoy4m -i t -a 10:11 -r
30000:1001 | mpeg2enc -f 8 newvideo.m2v'

   You can decode the audio as described in the `Transcoding of
existing MPEG-2' Section.


File: mjpeg-howto.info,  Node: Other things to know,  Prev: Decoding MPEG2 streams with mpeg2dec,  Up: Creating videos from other sources

4.4 Other things to know
========================

If you have Transport Streams from your DVB card, or os Satelite
Receiver you might want to demultiplex or cut them. A nice tool for
that is `Project X' available from:
http://www.lucike.info/page_projectx.htm

   You can process the streams afterwards as you would do with any mpeg
movie or demultiplexed audio video. So the `Transcoding of existing
MPEG-2' section of this document will be of interest.


File: mjpeg-howto.info,  Node: Checking if recording was successful,  Next: Edit the video,  Prev: Creating videos from other sources,  Up: Top

5 Checking if recording was successful
**************************************

You can use lavplay or glav. `IMPORTANT: NEVER' try to run xawtv and
lavplay or glav with hardware playback, it will not work. For software
playback it works fine.

   `>lavplay -p S record.avi'

   You should see the recorded video and hear the sound. But the
decoding of the video is done by the CPU which will place a heavy load
on the system.  The advantage of this method is you don't need xawtv.

   The better way:

   `>lavplay -p H record.avi'

   The video is decoded and played by the hardware. The system load is
now very low. This will play it back on-screen using the hardware
rather than software decoding.

   You might also try:

   `> lavply -p C record.avi'

   Which will play it back using the hardware but to the video output of
the card.

   `> glav record.avi'

   Does the same as lavplay but you have an nice GUI. The options for
glav and lavplay are nearly the same. Using no option SW playback is
used.

   Using hardware playback a signal for the Composite and SVHS OUT is
generated so you can view the movie on your TV.

   `> lav2yuv test.eli | yuvplay'

   Is a other way to get the video without sound. You can use yuvplay
once in the encoding command. When you use yuvplay in the encoding
command you see the changes made by filters and scaling. You can also
use it for slow-motion debugging.

   `NOTE:' After loading the driver's you have to start xawtv to set up
some things lavplay and glav do not, but they are needed for
HW-Playback. Don't forget to close xawtv !!

   `NOTE2:' Do not try to send glav an lavplay into background, wont
work correct !!!

   `NOTE3:' SECAM playback is now (12.3.2001) only in monochrome, but
the recording and encoding is done right.

   `NOTE4:'Bad cables may reduce the quality of the image. Normally you
can't see this but when there is text you might notice a small shadow.
When you see this you should change the cable.

   `Coming soon:' There is a tool which makes recoding videos very
simple: Linux Studio. You can download it at: http://ronald.bitfreak.net


File: mjpeg-howto.info,  Node: Edit the video,  Next: Converting the stream to MPEG or DIVx videos,  Prev: Checking if recording was successful,  Up: Top

6 Edit the video
****************

* Menu:

* Edit with glav::
* Unify videos::
* Separate sound::
* Separate images::
* Creating movie transitions::


File: mjpeg-howto.info,  Node: Edit with glav,  Next: Unify videos,  Up: Edit the video

6.1 Edit with glav
==================

Most tasks can be easily done by glav. Like deleting parts of the video,
cut paste and copy parts of the videos.

                        glav button description

   The modifications should be saved because glav does not
destructively edit the video. This means that the original video is
left untouched and the modifications are kept in an extra "Edit List"
file readable with a text editor. These files can be used as an input
to the other lavtools programs such as lav2wav, lav2yuv, lavtrans.

   If you want to cut off the beginning and the end of the stream mark
the beginning and the and, and use the "save select" button. The edit
list file is than used as input for the lavtools. If you want to split
a recorded video to some smaller parts simply select the parts and then
save each part to a different listfile.

   You can see all changes to the video and sound NOW and you do not
need to recalculate anything.

   If you want to get a "destructive" version of your edited video use:

   `> lavtrans -o short_version.avi -f a editlist.eli'

`-o'
     specifies the output name

`-f a'
     specifies the output format (AVI for example)

`editlist.eli'
     is the list file where the modifications are described.  You
     generate the list file with the "save all" or "save select"
     buttons in glav.



File: mjpeg-howto.info,  Node: Unify videos,  Next: Separate sound,  Prev: Edit with glav,  Up: Edit the video

6.2 Unify videos
================

`> lavtrans -o stream.qt -f q record_1.avi record_2.avi ...
record_n.avi'

`-o'
     specifies the outputfile name

`-f q'
     specifies the output format, quicktime in this case


   This is usually not needed. Keep in your mind that there is the 2GB
file-size-limit on 32Bit systems with an older glibc. Usually not a
problem these days


File: mjpeg-howto.info,  Node: Separate sound,  Next: Separate images,  Prev: Unify videos,  Up: Edit the video

6.3 Separate sound
==================

`> lavtrans -o sound.wav -f w stream.avi'

   Creates a wav file with the sound of the stream.avi Maybe needed if
you want to remove noise or if you want to convert it to another sound
format.

   Another way to split the sound is:

   `> lav2wav editlist.eli >sound.wav'


File: mjpeg-howto.info,  Node: Separate images,  Next: Creating movie transitions,  Prev: Separate sound,  Up: Edit the video

6.4 Separate images
===================

`>mkdir jpg; lavtrans -o jpg/image%05d.jpg -f i stream.avi'

   First create the directory "jpg". Then lavtrans will create single
JPG images in the jpg directory from the stream.avi file. The files
will be named: image00000.jpg, image00001.jpg ....

   The jpg images created contain the whole picture. But if you have
recorded at full size the images are stored interlaced. Usually the
picture viewers show only the first field in the jpg file.

   If you want to have the image in a single file you can use that
version

   `> lav2yuv -f 1 stream.avi | y4mtoppm -L >file.pnm'

   If you want to split the fields into single files use that:

   `>  lav2yuv -f 5 ../stream.avi | y4mtoppm | pnmsplit - image%d.pnm'

   Maybe interesting if you need sample images and do not want to play
around with grabbing a single image.


File: mjpeg-howto.info,  Node: Creating movie transitions,  Prev: Separate images,  Up: Edit the video

6.5 Creating movie transitions
==============================

Thanks to Philipp Zabel's lavpipe, we can now make simple transitions
between movies or combine multiple layers of movies.

   Philipp wrote this HOWTO on how to make transitions:

   Let's assume simple this scene: We have two input videos intro.avi
and epilogue.mov and want to make intro.avi transition into
epilogue.mov with a duration of one second (that is 25 frames for PAL
or 30 frames for NTSC).

   Intro.avi and epiloque.mov have to be of the same format (the same
frame rate and resolution). In this example they are both 352x288 PAL
files. intro.avi contains 250 frames and epilogue.mov is 1000 frames
long.

   Therefore our output file will contain:

`'
     the first 225 frames of intro.avi

`'
     a 25 frame transition containing the last 25 frames of intro.avi
     and the first 25 frames of epilogue.mov

`'
     the last 975 frames of epilogue.mov


   We could get the last 25 frames of intro.avi by calling:

   `>lav2yuv -o 225 -f 25 intro.avi'

   `-o 255', the offset, tells lav2yuv to begin with frame # 225 and `
-f 25' makes it output 25 frames from there on.

   Another possibility is:

   `> lav2yuv -o -25 intro.avi'

   Since negative offsets are counted from the end.

   And the first 25 frames of epilogue.mov:

   `> lav2yuv -f 25 epilogue.mov'

   `-o' defaults to an offset of zero

   But we need to combine the two streams with lavpipe. So the call
would be:

   `> lavpipe "lav2yuv -o 255 -f 25 intro.avi" "lav2yuv -f 25
epilogue.mov" '

   The output of this is a raw yuv stream that can be fed into
transist.flt.

   transist.flt needs to be informed about the duration of the
transition and the opacity of the second stream at the beginning and at
the end of the transition:

`-o num'
     opacity of second input at the beginning [0-255]

`-O num'
     opacity of second input at the end [0-255]

`-d num'
     duration of transition in frames


   An opacity of 0 means that the second stream is fully transparent
(only stream one visible), at 255 stream two is fully opaque.

   In our case the correct call (transition from stream 1 to stream 2)
would be:

   `> transist.flt -o 0 -O 255 -d 25'

   The -s and -n parameters equate to the -o and -f parameters of
lav2yuv and are only needed if anybody wants to render only a portion
of the transition for whatever reason. Please note that this only
affects the weighting calculations - none of the input is really
skipped.  If you use the skip parameter (-s 30, for example) you also
need to skip the first 30 frames in lav2yuv (-o 30) in order to get the
expected result. If you didn't understand this send an email to the
authors or simply ignore -s and -n. The whole procedure will eventually
be automated.

   Now we want to compress the yuv stream with yuv2lav:

   `> yuv2lav -f a -q 80 -o transition.avi'

   Reads the yuv stream from stdin and outputs an avi file (-f a) with
compressed jpeg frames of quality 80.

   Now we have the whole command for creating a transition:

   `> ypipe "lav2yuv -o 255 -f 25 intro.avi" "lav2yuv -f 25
epilogue.mov" | transist.flt -o 0 -O 255 -d 25 | yuv2lav -f a -q 80 -o
transition.avi'

   The resulting video can be written as a LAV Edit List, a plain text
file containing the following lines:

     LAV Edit List
     PAL
     3
     intro.avi
     transition.avi
     epilogue.mov
     0 0 224
     1 0 24
     2 25 999

   This file can be fed into glav or lavplay, or you can pipe it into
mpeg2enc with lav2yuv or combine the whole stuff into one single mjpeg
file with lavtrans or lav2yuv|yuv2lav.


File: mjpeg-howto.info,  Node: Converting the stream to MPEG or DIVx videos,  Next: Optimizing the stream,  Prev: Edit the video,  Up: Top

7 Converting the stream to MPEG or DIVx videos
**********************************************

First there is some general description in the encoding process and
afterwards there is a detailed description of some commonly used output
formats.

   If you want a one command conversation to mpeg videos try lav2mpeg in
the scripts directory

   The encoding with the lav2mpeg script looks like this for mpeg1
output:

   `>lav2mpeg -a 160 -b 2110 -d 320x240 -m mpeg1 -o output.mpg file.eli'

   * Will create a mpeg1 with videobitrate of 2110kBit/sec and
     audiobitrate of 160 kBit/sec

   * at a resolution of 320x240

   Or for the generation of mpeg2 output:

   `lav2mpeg -o mpeg2 -O output.mpg file.eli'

   * Will create a mpeg2 with default bitrate in same resolution as the
     input resolution

   Better results can be accomplished, however, by trying various
options and find out which ones work best for you. These are discussed
below.

   The creation of MPEG1 movies is explained with more examples and in
greater detail because most of the things that can be used for MPEG1
also work for the other output formats

   For the creation of of VCD/SVCD Stills sequences (-f 6, -f 7 in
mpeg2enc) you should see: http://www.mir.com/DMG/ Still sequences are
needed for the creation of menus in VCD/SVCD. The creation of menus is
described in the doku of vcdimager.

* Menu:

* Creating sound::
* Converting video::
* Putting the streams together::
* Creating MPEG1 Videos::
* Creating MPEG2 Videos::
* Creating Video-CD's::
* Creating SVCD::
* Creating DVD's::
* Creating DIVX Videos::


File: mjpeg-howto.info,  Node: Creating sound,  Next: Converting video,  Up: Converting the stream to MPEG or DIVx videos

7.1 Creating sound
==================

MPEG-1 videos need MPEG1-layer2 sound files. For MPEG-2 videos you can
use MPEG1-Layer2 and MPEG1-Layer3 (MP3).    Layer 3 (MP3) audio is not
an offically valid audio format but many VCD players will recognize it.
 MP3 audio is not valid for DVDs.  You should stick to MPEG1-Layer2
because most of the MPEG2 players (DVD Player for example usually the
different Winxx Versions have great problems with this too) are not
able to play MPEG2-Video and MPEG1-Layer3 sound.

   mp2enc is a MPEG1-layer 2 Audio encoder. The toolame encoder is also
able to produce an layer 2 file. You can use that one as well.
Toolame is much faster than mp2enc but toolame does not peform
resampling (48000 to 44100 samples/second).  Many hardware players will
play SVCDs using 48000 rate audio.  For mp3 creation I'm be sure you
have an encoder.

   Example:

   `> lav2wav stream.avi | mp2enc -o sound.mp2'

   This creates a mpeg sound file out of the stream.avi with 224kBit/sec
bitrate and a sample rate of 48kHz. If you audio file has 44.1kHz mp2enc
resamples the audio to create a 48kHz output. If you want a 44.1kHz
output sample rate you have to add -r 44100 to the mp2enc command

   Example

   `> cat sound.wav | mp2enc -v 2 -V -o sound.mp2'

   This creates a VCD (-V bitrate=224, stereo, sampling rate:44100)
compatible output from the wav file.

   With -v 2 mp2enc is more verbose, while encoding you see the number
of sec of audio already encoded.

   You can test the output with:

   `> plaympeg sound.mp2'

   `NOTE:' plaympeg is a MPEG1 Player for Linux, you can use other
players as well, for MPEG audio testing you can also use mpg123.


File: mjpeg-howto.info,  Node: Converting video,  Next: Putting the streams together,  Prev: Creating sound,  Up: Converting the stream to MPEG or DIVx videos

7.2 Converting video
====================

You can create MPEG1 and MPEG2 videos.

   Normally the first video you create is not the best. For optimal
quality/size you need to play with the bitrate, search radius, noise
filter .... The options of mpeg2enc are described in the manpage of
mpeg2enc.

   Example:

   `lav2yuv stream.avi stream1.avi | mpeg2enc -o video.m1v'

   This creates an video file with the default constant bitrate of
1152kBit/sec.  This is the bitrate you need if you want to create VCDs.
You can specify more files and also use the placeholder %nd. Where `n'
describes the number. By default mpeg2enc assumes that you want to
encode a not interlaced video to Mpeg-1. If you want to encode a full
size video with interlacing that command will fail.

   Example:

   `> lav2yuv streami%02d.avi | mpeg2enc -b 1500 -r 16 -o video.m1v'

   mpeg2enc creates a video with a bitrate of 1500kBit/s uses an search
radius of 16. That means when trying to find similar 16*16 macroblocks
of pixels between frames the encoder looks up to 16 pixels away from
the current position of each block. It looks twice as far when
comparing frames 1 frame apart and so on. Reasonable values are 16 or
24. The default is 16 so adding the option here is silly.  Lower values
(0, 8), improve the encoding speed but you get lower quality (more
visible artifacts) while higher values (24, 32) improve the quality at
the cost of the speed. With the file description of stream%02d.avi all
files are processed that match this pattern with 00, 01....

* Menu:

* Scaling::


File: mjpeg-howto.info,  Node: Scaling,  Up: Converting video

7.2.1 Scaling
-------------

Using yuvscaler one can now also scale the video before encoding it.
This can be useful for users with a DC10 or DC10+ cards which captures
at -d 1 768x576 or -d 2 384x288 (PAL/SECAM) or -d 1 640x480 (NTSC).

   You get a full description of all commands by reading the manpage or
running:

   `>yuvscaler -h'

   Example:

   `> lav2yuv stream.avi | yuvscaler -O VCD | mpeg2enc -o video.m1v'

   This will scale the stream to VCD size which for PAL/SECAM is
352x288 and for NTSC is 352x240. The scaled yuvstream is encoded to
MPEG-1.

   It can also do SVCD scaling to 480x480 (NTSC) or 480x576 (PAL/SECAM):

   `> lav2yuv stream.avi | yuvscaler -O SVCD -M BICUBIC | mpeg2enc -o
video.m1v'

   The mode keyword (-M) forces yuvscaler to use the higher quality
bicubic algorithms for downscaling and not the default resample
algorithms. Upscaling is always done using the bicubic algorithm.

   Example

   `> lav2yuv stream.avi | yuvscaler -I USE_450x340+20+30 -O
SIZE_320x200 | mpeg2enc -o video.m1v '

   Here we only use a part of the input and specify a nonstandard output
resolution.

   `NOTE:' yuvscaler can set a active area, and set everything else to
black using: -I ACTIVE_WidthxHeight+WidthOffset+HeightOffset

   Testing is done by:

   `> plaympeg video.m1v'

   `NOTE:'These are only examples. There are more options you can use.
You can use most of them together to create high quality videos with the
lowest possible bitrate.

   `NOTE2:'The higher you set the search radius the longer the
conversion will take. In general the more options used the longer
encoding takes.

   `NOTE3:'MPEG1 was not designed to be a VBR (variable bitrate stream)
!!  So if you encode with -q 15 mpeg2enc sets the maximal bitrate -b to
1152. If you want a VBR MPEG1 you have to set -b very high (2500).

   `NOTE4:'Maybe you should give better names than video.mpg. A good
idea is to use the options as part of the filename (for example:
`video_b1500_r16_41_21.m1v').  Another possibility is to call all the
layer 2 files ".mp2" all the MPEG-1 video files ".m1v" and all MPEG-2
video files ".m2v" Easy to see what's happening then. Reserve .mpg for
multiplexed MPEG-1/2 streams.


File: mjpeg-howto.info,  Node: Putting the streams together,  Next: Creating MPEG1 Videos,  Prev: Converting video,  Up: Converting the stream to MPEG or DIVx videos

7.3 Putting the streams together
================================

Example:

   `> mplex sound.mp2 video.m1v -o my_video.m1v'

   Puts the sound.mp2 and the video.m1v stream together to my_video.mpg

   Now you can use your preferred MPEG player and watch it. All players
(gtv for example) based on the SMPEG library work well for MPEG-1.
Other players (which can play MPEG-2 as well as MPEG-1 movies) are:
xmovie, xine, and MPlayer VLC, to name some.

   `NOTE:' If you have specified the `-S' option for mpeg2enc mplex
will automatically split the files if there is in the output filename a
%d (looks like: -o test%d.mpg) The files generated this way are
separate stand-alone MPEG steams!

   `NOTE2:' xine might have a problem with seeking through videos.
mplayer has a problem with the "seek backward/forward" with variable
bitrate streams because it goes forward in the file the amount of data
for a constant bitrate stream. That amount might be significantly more
than 10 seconds or one minute (those are the amount mplayer seeks for
each press of the arrow keys). So don't wonder if it seeks much more
time forward or backward than you expect.

   `Variable bit-rate multiplexing:' Remember to tell mplex you're
encoding VBR (-V option) as well as mpeg2enc (see the example scripts).
It *could* auto-detect but it is not working yet. You should tell mplex
a video buffer size at least as large as the one you specified to
"mpeg2enc" Sensible numbers for MPEG-1 might be a ceiling bit-rate of
2800Kbps, a quality ceiling (quantization floor) of 6 and a buffer size
of 400K.

   Example:

   `> mplex -V -r 1740 audio.mp2 video_vbr.m1v -o vbr_stream.mpg'

   Here we multiplex a variable bitrate stream. mplex is now a single
pass multiplexer so it can't detect the maximal bitrate and we have to
specify it. The data rate for the output stream is: audio bitrate +
peak videobitrate + 1-2% for mplex information. If audio (-b 224) has
224kBit, video has 1500kBit (was encoded with -b 1500 -q 9) then we
have 1724 * 1.01 or about 1740kBit.

   Example:

   `> plaympeg my_video.mpg'

   or

   `> mplayer my_video.mpg'


File: mjpeg-howto.info,  Node: Creating MPEG1 Videos,  Next: Creating MPEG2 Videos,  Prev: Putting the streams together,  Up: Converting the stream to MPEG or DIVx videos

7.4 Creating MPEG1 Videos
=========================

For MPEG1 you can use mpeg layer 2 Audio and mpeg1 video. A subset of
MPEG1 movies are VCD's. You can use VBR (Variable BitRate) for the
Video (although VCDs are almost always use CBR video) but the Audio has
to be CBR (Constant BitRate).

   MPEG1 is recommended for picture sizes up to 352x288 for PAL and
352x240 for NTSC for larger sizes MPEG2 is the better choice.  There is
no exact resolution where MPEG1 is better than MPEG2.  Just to make
soure, MPEG1 can't handle interlaced sources. If you video is
interlaced you need MPEG2 to get it proper encoded.

* Menu:

* MPEG1 Audio creation Example::
* MPEG1 Video creation Example::
* MPEG1 Multiplexing Example::


File: mjpeg-howto.info,  Node: MPEG1 Audio creation Example,  Next: MPEG1 Video creation Example,  Up: Creating MPEG1 Videos

7.4.1 MPEG1 Audio creation Example
----------------------------------

`> lav2wav editlist.eli | mp2enc -r 44100 -o sound.mp2'

   You can save some bits by telling mp2enc to use a lower bitrate (-b
option) like 160 or 192 kBit/s.  The -r 44100 option forces mp2enc to
generate a 44.1kHz audio file.

   `> lav2wav editlist.eli | mp2enc -b 128 -m -o sound.mp2'

   This creates a mono output with an bitrate of 128kBit/sec bitrate.
The input this time is the editlistfile (can have any name) created
with glav so all changes you made in glav are direct processed and
handed over to mp2enc.  You do NOT have to create an edited stream with
lavtrans to get it converted properly.


File: mjpeg-howto.info,  Node: MPEG1 Video creation Example,  Next: MPEG1 Multiplexing Example,  Prev: MPEG1 Audio creation Example,  Up: Creating MPEG1 Videos

7.4.2 MPEG1 Video creation Example
----------------------------------

`> lav2yuv editlist.eli | mpeg2enc -b 2000 -r 24 -q 6 -o video.m1v'

   mpeg2enc creates an video with an bitrate of 2000kBit/s (or
2048000Bit/s) but the -q flag activates the variable bitrate and a
quality factor of 6. It uses a search radius of 24.

   `Explanation:'when mpeg2enc is invoked without the 'q' flag it
creates "constantbit-rate" MPEG streams. Where (loosely speaking) the
strength of compression (and hence picture quality) is adjusted to
ensure that on average each frame of video has exactly the specified
number of bits. Such constant bit-rate streams are needed for
broadcasting and for low-cost hardware like DVD and VCD players which
use slow fixed-speed player hardware.

   Obviously this is fairly inefficient as it means inactive scenes use
up bits that could better be "spent" on rapidly changing scenes.
Setting the 'q' flag tells mpeg2enc to generate variable bit-rate
streams. For such streams the bit-rate specified is simply the maximum
permissible. The 'q' parameter specifies the minimum degree of
compression to be applied by specifying how exactly picture information
is recorded. Typically, 'q' would be set so that quiet scenes would use
less than the specified maximum (around 6 or 8) but fast moving scenes
would still be bit-rate limited. For archival purposes setting a
maximum bit-rate high enough never to be reached (e.g. 10Mbps) and a q
of 2 or 3 are reasonable choices.

   Example:

   `> lav2yuv stream.avi | yuvscaler -I ACTIVE_352x240+0+24 | mpeg2enc
-b 1152 -r 16 -4 1 -2 1 -o video.m1v'

   Usually there is at the top and at the bottom a nearly black border
and a lot of bandwidth is used for something you do not like. The
yuvscaler -I ACTIVE option sets everything that is not in the described
area to black, but the imagesize (352x288) is not changed.  So you have
a real black border the encoder only uses a few bits for encoding them.
You are still compatible with the VCD's format in this example.  To
determine the active window extract one frame to the jpeg format:

   `> lavtrans -f i -i 100 -o frame.jpg test.avi'

   Than use your favorite graphic display program to determine the
active size.  The -4 1 and -2 1 options improves the quality about 10%
but conversion is slower.

   At the size of 352x288 (1/2 PAL size, created when using the -d 2
option when recording) the needed bitrate is/should be between 1000 -
1500kBit/s. For NTSC it should be about the same, because the image is
smaller, but there are more frames per second than in PAL.

   Anyways, the major factor is quality of the original and the degree
of filtering. Poor quality unfiltered material typically needs a higher
rate to avoid visible artifacts.  If you want to reduce bit-rate
without annoying artifacts when compressing broadcast material you
should try one (or more) of the noise filters.

   Example:

   `> lav2yuv stream.avi | mpeg2enc -b 1500 -n s -g 6 -G 20 -P -o
video.m1v'

   Here the stream.avi will be encoded with:

`-b 1500'
     a Bitrate of 1500kBit/sec

`-n s'
     the input Video norm is forced to SECAM

`-P'
     This ensures that 2 B frames appear between adjacent I/P frames.
     Several common MPEG-1 decoders can't handle streams that do not
     have 2 B-frames between I/P frames

`-g 6 -G 20'
     the encoder can dynamically change the group-of-pictures size to
     reflect scene changes. This is done by setting a maximum GOP (-G
     flag) size larger than the minimum (-g flag).  For VCDs sensible
     values might be a minimum of 9 and a maximum of 15.  For SVCD 9
     and 15 would be good values. If you only want to play it back on
     SW player you can use other min-max values.


   Example

   `> lav2yuv stream*.avi | mpeg2enc -b 1500 -r 16 -4 1 -2 1 -S 630 -B
260 -o video_n1_1500_r16_41_21_S630_B240.m1v'

   lav2yuv processes all the stream files. Then mpeg2enc is given some
options that make the encoded stream look nicer. Using `-S 630' means
that mpeg2enc marks the stream so that mplex generates a new stream
every 630MB. One important thing is the use of the `-B' option which
specifies the non-video (audio and mplex information) bitrate. The `-B'
value of 260 should be fine for audio with 224kBit and mplex
information. For further information take a look at the encoding
scripts in the scripts directory.


File: mjpeg-howto.info,  Node: MPEG1 Multiplexing Example,  Prev: MPEG1 Video creation Example,  Up: Creating MPEG1 Videos

7.4.3 MPEG1 Multiplexing Example
--------------------------------

Example

   ` >mplex sound.mp2 video.m1v -o my_video.mpg'

   Puts the sound.mp2 and the video.m1v stream together to my_video.mpg.
It only works that easy if you have CBR (the -q option was not used with
mpeg2enc).

   Example

   `mplex -V -r 1740 audio.mp2 video_vbr.m1v -o vbr_stream.mpg'

   Here we multiplex a variable bitrate stream. mplex is now a single
pass multiplexer so it can't detect the maximal bitrate and we have to
specify it. The data rate for the output stream is: `audio bitrate +
peak videobitrate + 1-2% for mplex information'. If audio (-b 224) has
224kBit, video has 1500kBit (was encoded with -b 1500 -q 9) then we
have 1724 * 1.01 or about 1740kBit.


File: mjpeg-howto.info,  Node: Creating MPEG2 Videos,  Next: Creating Video-CD's,  Prev: Creating MPEG1 Videos,  Up: Converting the stream to MPEG or DIVx videos

7.5 Creating MPEG2 Videos
=========================

MPEG2 is recommended for sources with a greater picture than 352x240
for NTSC and 352x288 for PAL. MPEG2 can also handle interlaced sources
like recording from TV at full resolution.

   MPEG2 allows the usage of mpeg layer 3 (mp3) sound. So you can use
your favorite mp3encoder for the creation of the sound.  However, MP3
audio is not valid for DVDs.  It is best to use MP2 (Layer 2) audio.
The audio can also be a VBR Stream.

   MPEG2 is usually a VBR Stream. MPEG2 creation with optimization
requires a lot of CPU power.  A film with the double resolution is NOT
4 times larger than an MPEG1 Stream. Depending on your quality settings
it will be about 1.5 up to 3 times larger than the MPEG1 Stream at its
lower resolution.

* Menu:

* MPEG2 Audio creation Example::
* MPEG2 Video creation Example::
* MPEG2 Multiplexing Example::


File: mjpeg-howto.info,  Node: MPEG2 Audio creation Example,  Next: MPEG2 Video creation Example,  Up: Creating MPEG2 Videos

7.5.1 MPEG2 Audio creation Example
----------------------------------

`> lav2wav editlist.eli | mp2enc -o sound.mp2'

   This will fit the MPEG2 quite well. You can save some bits by telling
mp2enc to use a lower bitrate (-b option) like 160 or 192 kBit/s. And
might want to add -r 44100 so that mpeg2enc generates a 44.1kHz
sampling rate audio file. I hope I don't need to explain the usage of
an MP3 Encoder.  But you should not use all the fancy options that are
available.


File: mjpeg-howto.info,  Node: MPEG2 Video creation Example,  Next: MPEG2 Multiplexing Example,  Prev: MPEG2 Audio creation Example,  Up: Creating MPEG2 Videos

7.5.2 MPEG2 Video creation Example
----------------------------------

`> lav2yuv editlist.eli | mpeg2enc -f 3 -b 3000 -q 9 -o video.m2v'

   A very simple example for MPEG2 Video.  The most important option is
the -f 3. That tells mpeg2enc that it should create a MPEG2 stream.
Because it is a generic MPEG2 you have to use the -b bitrate options.
And should use the -q option because you usually want a space saving
VBR Stream. When using VBR streams the -b option tells mpeg2enc the
maximum bitrate that can be used. The -q option tell mpeg2enc what
quality the streams should have.  The bitrate has an upper bound of the
value specified by -b.

   `> lav2yuv editlist.eli | mpeg2enc -f 3 -4 1 -2 1 -q7 -b 4500 -V 300
-P -g 6 -G 18 -I 1 -o video.m2v'

   This will generate a higher quality MPEG2 stream because the -4 1 and
-2 1 options were used.  With -b 4500 -q 7 you tell mpeg2enc the
maximal bitrate and the quality factor.  -V is the video buffer size
used for decoding the stream. For SW playback it can be much higher
than the default. Dynamic GOP is set with -g and -G.  A larger GOP size
can help reduce the bit-rate required for a given quality but very
large sizes can introduce artifacts due to DCT/iDCT accumulated
rounding errors.  The -P option also ensures that 2 B frames appear
between adjacent I/P frames. The -I 1 option tells mpeg2enc that the
source is a interlaced material like videos. There is (time consuming)
interlaced motion compensation logic present in mpeg2enc.  Mpeg2enc
will use that logic if the size of the frames you encode is larger than
the VCD size for your TV Norm.

   If you deinterlacing the movie with yuvdeinterlace you should tell
mpeg2enc that it does not need to do motion estimation for interlaced
material. You have to use the -I 0 option of mpeg2enc to say that the
frames are already deinterlaced.  This will save a lot of time when
encoding. If you don't use -I 0 it will not cause problems, the
encoding will just take longer.

   You can also use scaling an options that optimize (denoise) the
images to get smaller streams.  These options are explained in detail
in the following sections.

* Menu:

* Which values should be used for VBR Encoding::
* Encoding destination TV (interlaced) or Monitor (progressive)::


File: mjpeg-howto.info,  Node: Which values should be used for VBR Encoding,  Next: Encoding destination TV (interlaced) or Monitor (progressive),  Up: MPEG2 Video creation Example

7.5.2.1 Which values should be used for VBR Encoding
....................................................

The -q option controls the minimum quantization of the output stream.
Quantization controls the precision with which image information is
encoded. The lower the value the better the image quality.  Values
below 4 are extremes and should only be used if you know what you are
doing

   Usually you have to set up a maximum bitrate with the -b option.
The tricky task is to set a value for the -q option and the -b option
that produces a nice movie without using too much bandwidth and does not
introduce too many artifacts.

   A quality factor should be chosen that way that the mplex output of
Peak bit-rate and average bit-rate differ by about 20-25%.  If the
difference is very small (less than < 10%) it is likely that you will
begin to see artifacts in high motion scenes.  The most common cause of
the average rate being too close (or equal) to the maximum rate is
wrong value for the maximal bitrate or a quality factor that is too
high.

   A combination that will produce more artifacts than you can count is
a SVCD with a maximal video bitrate of 2500kBit and a qualitfactor set
to 1 or 2.  For SVCD with a video limit of 2500kBit a quality factor of
7-11 fits quite good (8 is the default). If you use filter programs or
have a very good source like digital TV, DVD like material or rendered
pictures you can use a quality factor of 6 when creating SVCDs.  If
your SVCD/DVD player supports higher bitrates than the official
2788kBit/sec for the video and audio.   When using a higher bitrate and
quality factor action scenes will look much better but of course the
playing time of the disc will be less.

   The same (7-11) quality factor for a full size picture and a top
bitrate of 3500 to 4000 kBit will produce few artifacts.

   For SVCD/DVD you can expect a result like the one described if the
maximal bitrate is not set too low:

   q <= 6 real sharp pictures, and good quality    q <= 8 good quality
 q >= 10 average quality    q >= 11 not that good    q >= 13 here even
still sequences might look blocky


File: mjpeg-howto.info,  Node: Encoding destination TV (interlaced) or Monitor (progressive),  Prev: Which values should be used for VBR Encoding,  Up: MPEG2 Video creation Example

7.5.2.2 Encoding destination TV (interlaced) or Monitor (progressive)
.....................................................................

MPEG2 supports interlaced data in addition to the progressive format.
A MPEG2 movie can be interlaced or progressive. It depends on the source
(film or broadcast) and on the viewing device.

   If you encode a film both fields should be the same. Deinterlace the
stream with yuvdeinterlace, or if you have a high quality source, and
don't need to use the denoiser, with yuvcorrect -T NOT_INTERLACED. Also
set the mpeg2enc interlace-mode (-I) option to 0. This means that there
is no interlacing.  We do not really need deinterlacing here because
there is no motion between the fields of the frame. We only need to
unite the two fields into a single progressive frame.

   This movie should play back an any device (TV or Monitor) without
problems.

   If you have an interlaced source (broadcast) you can encode it as
interlaced stream. Or deinterlace the stream and encode it as
progressive stream. If you deinterlace it with yuvdeinterlace, you will
lose details.  But if you plan to play the recorded stream on your DVD
player and your TV it would not be wise to perform deinterlacing.  If
you only want to play it back on the Monitor (progressive display) the
picture looks better when playing it back if it is deinterlaced. If the
player you use can do deinterlacing it does not matter if your encoded
video has interlaced frames or progressive frames.

   If you plan to deinterlace the stream you can only do this with
yuvdeinterlace, and set the mpeg2enc -I 0. If you do not want to
deinterlace the stream you do not need to set any special option (do
not use yuvdeinterlace and mpeg2enc -I 0)

   If you like to pause the stream and look on the still you should
deinterlace. Because then the image is flicker free when pausing.

   If you have a film (progressive) with parts from a broadcast
(interlaced) mixed together (like in a documentary where some parts
from a speaker are recorded interlaced and other parts are filmed) you
have to choose between good film sequences with average still images or
average looking film sequences with good still images.

   For good film with average stills do not deinterlace.  For average
film sequences with good stills then deinterlace (using yuvdeinterlace
and mpeg2enc -I 0).


File: mjpeg-howto.info,  Node: MPEG2 Multiplexing Example,  Prev: MPEG2 Video creation Example,  Up: Creating MPEG2 Videos

7.5.3 MPEG2 Multiplexing Example
--------------------------------

`> mplex -f 3 -b 300 -r 4750 -V audio.mp3 video.m2v -o final.mpg'

   Now both streams (a mp3 audio and a mpeg2 video) are multiplex into a
single stream (final.mpg). You have to use the -f 3 option to tell
mplex the output format. You also have to add the -b decoder buffers
size with the same value used when encoding the video. -r is that rate
of video + audio +1-2% of mplex information.

   The -V option tells that your source for mplexing is a VBR stream. If
you don't use this option mplex creates something like a CBR Stream
with the bitrate you have told it with the -r option.  These streams
are usually get BIG.


File: mjpeg-howto.info,  Node: Creating Video-CD's,  Next: Creating SVCD,  Prev: Creating MPEG2 Videos,  Up: Converting the stream to MPEG or DIVx videos

7.6 Creating Video-CD's
=======================

VCD is a constrained version of MEPG1 streams.  VCD format was defined
by Philips. The goal was to use a single speed CD-drive and other cheap
hardware (not flexible) to have a cheap HW-Player.  Because of that
there are some limitations on VCD's.  The bitrate for video is 1152kBit
and for audio layer 2 audio 224kBit stereo.  You are not allowed to use
the -q option, dynamic GOP sizes and the video buffer is limited to
46kB.  The image size is limited to 352x240 for NTSC, an to 352x288 for
PAL.

   If you have no VCD (only) player and you plan to use your DVD player
then it is quite possible that the DVD player will be flexible enough
to allow higher bitrates, dynamic GOP sizes, larger video buffer and so
on

* Menu:

* VCD Audio creation Example::
* VCD Video creation Example::
* VCD Multiplexing Example::
* Creating the CD::
* Notes::
* Storing MPEGs::


File: mjpeg-howto.info,  Node: VCD Audio creation Example,  Next: VCD Video creation Example,  Up: Creating Video-CD's

7.6.1 VCD Audio creation Example
--------------------------------

`> lav2wav stream.avi | mp2enc -V -o sound.mp2'

   `-V' force VCD 2.0 compatible output.  There the audio samplerate is
fixed to 44.1kHz. And  you can choose the audio bitrate for mono audio
to be 64, 96 or 192kBit/sec. If you have stereo audio you can choose
128, 192, 224 or 384kBit/sec.  For hardware players, you should stick
to 44.1 224kBps Stereo layer 2 Audio.


File: mjpeg-howto.info,  Node: VCD Video creation Example,  Next: VCD Multiplexing Example,  Prev: VCD Audio creation Example,  Up: Creating Video-CD's

7.6.2 VCD Video creation Example
--------------------------------

`> lav2yuv stream.avi | yuvscaler -O VCD | mpeg2enc -f 1 -r 16 -o
video.mpg'

   For a VCD compatible output the -f 1 sets all options in mpeg2enc as
needed. It seems that many VCD players (Avex for example) are not able
to play MPEG streams that are encoded with a search radius greater than
16 so do not use the -r option to override the default of 16.

   `> lav2yuv streams.eli | mpeg2enc -f 1 -4 1 -2 1 -S 630 -B 260 -P -o
video.m1v'

   Using `'-S 630" means that mpeg2enc marks the stream so that mplex
generates a new stream every 630MB. One important thing is the use of
the `-B' option which specifies the non-video (audio and mplex
information) bitrate. The -B value of 260 should be fine for audio with
224kBit and mplex information. For further information take a look at
the encoding scripts in the scripts directory. So the multiplexed
streams should easily fit on a CD with 650MB.

   The default value (-B) is 700MB for the video. mpeg2enc marks
automatically every stream at that size if the -B option is not used to
set a different value.  If you have a CD where you can write more data
(perhaps as much as 800MB), you have to set the -S option or otherwise
mpeg2enc will mark the stream at 700 MB, and mplex will split the
stream there.  Which is almost certainly not what you want.


File: mjpeg-howto.info,  Node: VCD Multiplexing Example,  Next: Creating the CD,  Prev: VCD Video creation Example,  Up: Creating Video-CD's

7.6.3 VCD Multiplexing Example
------------------------------

`> mplex -f 1 sound.mp2 video.mpg -o vcd_out.mpg'

   The -f 1 option turns on a lot of weird stuff that otherwise has no
place in a respectable multiplexer!


File: mjpeg-howto.info,  Node: Creating the CD,  Next: Notes,  Prev: VCD Multiplexing Example,  Up: Creating Video-CD's

7.6.4 Creating the CD
---------------------

The multiplexed streams have to be converted to an VCD compatible.
This is done by vcdimager http://www.vcdimager.org/

   `> vcdimager testvideo.mpg'

   Creates a `videocd.bin', the data file, and a `videocd.cue' which is
used as control file for cdrdao.

   You use cdrdao to burn the image. Cdrdao is yet another fine
Sourceforge project which is found at: http://cdrdao.sourceforge.net/


File: mjpeg-howto.info,  Node: Notes,  Next: Storing MPEGs,  Prev: Creating the CD,  Up: Creating Video-CD's

7.6.5 Notes
-----------

For MPEG-1 encoding a typical (45 minute running time) show or 90 odd
minute movie from an analog broadcast a constant bit-rate of around
1800 kBit/sec should be ideal. The resulting files are around 700M for
45 minutes which fits nicely as a raw XA MODE2 data track on a CD-R.
For pure digital sources (DTV or DVD streams and similar) VCD 1152
works fine.

   `Note:' If you encode VBR MPEG1 (-q) remember the Hardware was
probably not designed to do the playback because it is not in the
specifications. If it works be very happy. I've noticed that it helps
when you have an MPEG1 Stream to tell vcdimager that it is an SVCD.
vcdimager complains (but only with a warning and not a fatal error) but
you should be able to burn it. This could convince the player to use
different routines in its firmware and play it back correct, but there
is no guarantee of that.


File: mjpeg-howto.info,  Node: Storing MPEGs,  Prev: Notes,  Up: Creating Video-CD's

7.6.6 Storing MPEGs
-------------------

If you record the data as XA mode 2 tracks you can fit appreciably more
on a CD (at the expense of error correction/detection). You can use
vcdimager to do this and vcdxrip (part of the vcdimager package) to
extract ("rip") the resulting files. For better Quality there are SVCD
and XVCD and DVD.

   Currently SVCD is fully supported with a pre-set format in mplex and
tools to create disks. MPEG streams that can be played by DVD player
hardware and software can readily produced using mpeg2enc/mplex

   If your player doesn't support SVCD you may well find it can handle
VCD streams that have much higher than standard bit-rates. Often as
much as 2500kBit/sec is possible. The several brands of DVD players can
also play wilding out of spec SVCD and VCD discs.  With higher
bit-rates and good quality source material it is worth trying
mpeg2enc's -h flag which produce a stream that is as sharp as the
limits of the VCD standard permits.

   However, if your player supports it and you have the patience for the
longer encoding times SVCD is a much better alternative. Using a more
efficient MPEG format SVCD more than doubles VCD's resolution while
typically producing files that are less than twice as big.


File: mjpeg-howto.info,  Node: Creating SVCD,  Next: Creating DVD's,  Prev: Creating Video-CD's,  Up: Converting the stream to MPEG or DIVx videos

7.7 Creating SVCD
=================

Super Video CD (SVCD) is an enhancement to Video CD that was developed
by a Chinese government-backed committee of manufacturers and
researchers.  The final SVCD spec was announced in September 1998.  A
good explanation of the SVCD format from Philips can be found here:
http://lipas.uwasa.fi/~f76998/video/svcd/overview/.

   Record at full TV resolution (means: -d 1 for PAL this is 720x576)
The resolution is for NTSC is 480x480 of PAL 480x576, so you know why
you should record at full size.

* Menu:

* SVCD Audio creation Example::
* SVCD Video creation Example::
* SVCD Multiplexing Example::
* SVCD Creating the CD::


File: mjpeg-howto.info,  Node: SVCD Audio creation Example,  Next: SVCD Video creation Example,  Up: Creating SVCD

7.7.1 SVCD Audio creation Example
---------------------------------

`> lav2wav stream.avi | mp2enc -V -e -o sound.mp2'

   The SVCD specifications permit a much wider choice of audio rates,
it is not necessary to use 224 kBit/sec. Any audio rate between 32 and
384 kBit/sec is permitted. The audio may be VBR (Variable Bit Rate).
The -e enables the CRC error protection for the audio. The CRC has to
be enabled to be SVCD conform. But it seems that most players don't pay
attention to the CRC information. The CRC information need 2 bytes per
Audio frame

   The approximate frame length formula for MPEG-1 layer-II is:

   [frame length in bytes) = 144 * (byte rate) / (sample rate]

   If you have the typical VCD settings the CRC data needs about 0,27%
of the whole data. In the worst case, where you have a MONO 32k Bitrate
stream, the CRC data needs 1,92%.


File: mjpeg-howto.info,  Node: SVCD Video creation Example,  Next: SVCD Multiplexing Example,  Prev: SVCD Audio creation Example,  Up: Creating SVCD

7.7.2 SVCD Video creation Example
---------------------------------

`> lav2yuv stream.avi | yuvscaler -O SVCD | mpeg2enc -f 4 -q 7 -I 1 -V
200 -o video.m2v'

`-f 4'
     sets the options for mpeg2enc to SVCD

`-q 7'
     tell mpeg2enc to generate a variable bitrate stream

`-I 1'
     tell mpeg2enc to assume that the original signal is field
     interlaced video where the odd rows of pixels are sampled a half
     frame interval after the even ones in each frame. The -I 0
     (progressive output (no field pictures)) option will also work for
     PAL


   You can use lower bitrates, but the SVCD standard limits `total
bit-rate (audio and video) to 2788800 Bit/sec'. So with 224Kbps audio
and overhead 2550 may already be marginally too tight. Since the SVCD
format permits any audio rate between 32 and 384 kBit/sec you can save
a few bits/sec by using 192k audio (or for non-musical material 160k).

   SVCD supports variable bitrate (VBR), because MPEG2 is usually VBR,
but with the top video bitrate limit of 2500kBit/sec. With the -f 4
flag the encoder also sets dynamic GOP with a low limit of -g 6 and a
high limit of -G 18. This saves a few bits/sec and improves the picture
quality during scene changes.  When encoding with -f 4 mpeg2enc ignores
the video bitrate (-b) and search radius (-r) options. If you use -f 5
you have to specify the bitrate and other options to mpeg2enc.

   Another possibility for movies in PAL (European style 25 frames/50
fields per sec) video is:

   `> lav2yuv stream.avi | yuvscaler -O SVCD | mpeg2enc -f 4 -I 0 -V
300 -o video.m2v'

   Movies are shot on film at 24 frames/sec. For PAL broadcast the film
is simply shown slightly "too fast" at 25 frame/sec (much to the pain
of people with an absolute pitch sense of pitch). The -I 0 flag turns
off the tedious calculations needed to compensate for field interlacing
giving much faster encoding.

   Unfortunately, movies broadcast in NTSC (US style 30 frames/60 fields
sec) video this will produce very poor compression. The "pulldown"
sampling used to produce 60 fields a second from a 24 frame a second
movie means half the frames in an NTSC *are* field interlaced.

   Don't forget the -S and -B options mentioned above. You want the
stream to fit on a CD don't you ?


File: mjpeg-howto.info,  Node: SVCD Multiplexing Example,  Next: SVCD Creating the CD,  Prev: SVCD Video creation Example,  Up: Creating SVCD

7.7.3 SVCD Multiplexing Example
-------------------------------

`> mplex -f 4 -b 300 -r 2750 sound.mp2 video.m2v -o svcd_out.mpg'

`-f 4'
     tells mplex to mplex a SVCD

`-r 2750'
     is the calculated Audio + Video Bitrate + 1-2% multiplex
     information

`-b 300'
     is the buffer available on the playback device (the same value as
     used for the video encoding (mpeg2enc's -V option).



File: mjpeg-howto.info,  Node: SVCD Creating the CD,  Prev: SVCD Multiplexing Example,  Up: Creating SVCD

7.7.4 SVCD Creating the CD
--------------------------

Example:

   `> vcdimager -t svcd testvideo.mpg'

   Creates a `videocd.bin', the data file, and a `videocd.cue' which is
used as control file for cdrdao.

   Use cdrdao to burn the image as mentioned earlier.

   `NOTE:'If you want to build "custom" VCD/SVCD you will need to use
the mplex -f 2 and -f 5 switches.

   `NOTE:'The VCD and SVCD stuff may work on your HW player or not.
There are many reports that it works quite well. Don't be worried if it
does not work. Nor am I responsible for unusable CDs. ("coasters")


File: mjpeg-howto.info,  Node: Creating DVD's,  Next: Creating DIVX Videos,  Prev: Creating SVCD,  Up: Converting the stream to MPEG or DIVx videos

7.8 Creating DVD's
==================

That statement was correct a few years ago: Everything in this section
is very new. So it can change every day.  The limitations I mention
here might not exist in the current version.  Currently (Dec. 2007) DVD
creating is working.

   You need obviously a DVD writer. I own a Ricoh DVD+RW that works,
and I know of a DVD-RAM writer that is able to to burn DVD-R. That
disks also work with a DVD-Player. Which programs you use for burning
depends on the DVD writer drive.

   For the creation and writing of the VOB, IFO and BUP files we use
dvdauthor. Aviable from Sourceforge (you might have guessed it)
http://dvdauthor.sourceforge.net.

* Menu:

* DVD Audio creation Example::
* DVD Video creation Example::
* DVD Multiplexing Example::
* DVD creation Example::


File: mjpeg-howto.info,  Node: DVD Audio creation Example,  Next: DVD Video creation Example,  Up: Creating DVD's

7.8.1 DVD Audio creation Example
--------------------------------

`> lav2wav stream.eli | mp2enc -o sound.mp2'

     The sample rate has to be 48kHz. The mp2enc does create by default
     a sample rate of 48kHz. If it is not a 48kHz mp2enc will resample
     the audio to get the sample rate.  If the audio is recorded at
     48kHz then no resampling is needed and toolame can be used for the
     encoding (it is faster than mp2enc).



File: mjpeg-howto.info,  Node: DVD Video creation Example,  Next: DVD Multiplexing Example,  Prev: DVD Audio creation Example,  Up: Creating DVD's

7.8.2 DVD Video creation Example
--------------------------------

`> lav2yuv stream.eli | mpeg2enc -f 8 -o video.m2v'

`-f 8'
     This sets the options correctly for a MPEG-2 video that is
     compliant with the DVD standard.  The maximum bitrate is set to
     7500kBps and the video buffer size is set to 230KB. The default
     quality factor is set to 8.  mpeg2enc sets currenty no automatic
     sequence length as it does for VCD/SVCD.


   The other options to get a low bitrate and high quality stream can
also be used to override the default settings mentioned above.  You can
also use yuvdenoise to increase the picture quality if the input data is
noisy (from a VHS tape for example).  A typical command will look like
this:

   `lav2yuv moby.eli | yuvdenoise | mpeg2enc -f 8 -q 7 -4 1 -2 1 -P -I
0 -N -o video_DVD.m2v'


File: mjpeg-howto.info,  Node: DVD Multiplexing Example,  Next: DVD creation Example,  Prev: DVD Video creation Example,  Up: Creating DVD's

7.8.3 DVD Multiplexing Example
------------------------------

`> mplex -f 8 sound.mp2 video.m2v -o my_dvdlikestream.mpg'

`-f 8'
     Here again we specify that we want to have DVD like MPEG stream.
     mplex cannot do all the fancy things allowed for a DVD, but it is
     close enough that the HW-DVD players accept it.

`-o'
     there we specify the output filename.



File: mjpeg-howto.info,  Node: DVD creation Example,  Prev: DVD Multiplexing Example,  Up: Creating DVD's

7.8.4 DVD creation Example
--------------------------

This topic will be covered by the documentation of the dvdauthor
program.  For questions please see dvdauthor In general it will work
like this:

   `> dvdauthor -o output/ stream1.mpg stream2.mpg ...
my_dvdlikestream.mpg; dvdauthor -T -o output/ '

   You will get a directory with AUDIO_TS and VIDEO_TS directories.
Burning the data from the disk to a DVD+R/+RW writer would be done like
this:

   `growisofs -Z /dev/scd2 -dvd-video mydvd/'

   If you own a DVD+RW/+R drive a good place for more information is:
DVD+RW/+R for Linux page. You also need a version of the cdrtools with
`dvd-video' support.  The cdrtools 1.11a27 is known to work but newer
versions already exist.

   For other writers the commands to write a DVD will be different. You
can get some more information in the dvdauthor package. There is no
guarantee that it will work at all !!!


File: mjpeg-howto.info,  Node: Creating DIVX Videos,  Prev: Creating DVD's,  Up: Converting the stream to MPEG or DIVx videos

7.9 Creating DIVX Videos
========================

* Menu:

* lav2avi-sh::


File: mjpeg-howto.info,  Node: lav2avi-sh,  Up: Creating DIVX Videos

7.9.1 lav2avi-sh
----------------

Another way of creating DIVX is the program `mencoder' which is from
the mplayer project.  http://www.mplayer.hu/.  For more information
about mencoder please read mencoder/mplayer help and documents. A first
and a second pass give at the end of pass hints for bitrate which can
be used for encoding to specific size (650 MB, 700 MB and 800 MB). The
script lav2avi.sh uses this information if provided (for short streams
it is omitted by mencoder).  Look for parameter `preferedSize' in the
script. You can also specify other parameters used for encoding with
`encoderParam' option in the script. For a description of the usable
parameters take a look in the mplayer/mencoder manual.

   The outputfilename is that name of your input file (first option)
but with the extension avi. If the size of file is less then specified
by `preferedSize' it's because the source was of very high quality (no
noise) and the specified bitrate was higher than required.  You usually
get 700MB for 1.5 hour film at half image size with bitrate around 900
that means for divx good quality (assuming good quality source material
of course).

   The script does a 3 step encoding:

   * 1st step - audio encoding

   * 2nd step - first video pass

   * 3rd step - second video pass

   The mplayer/mencoder documentation deprecates the use of the 3 pass
encoding method (it can cause A/V sync problems) and recommends the use
of the 2 pass method.   The mencoder/mplayer documentation is extensive
and has many helpful hints (and a bitrate calculator in the TOOLS/
directory).

   For encoding use the fast ffmpeg (lavc) codec. It gives nice results
together with high good performance. For audio encoding mp3 is used.
For encoding of all parts it uses unix pipes. This mean that you DO NOT
need additional space on your hard drive where all glav manipulations
will be done. For audio encoding the script uses a FIFO queue.

   If you want to tweak the script for your own needs, use these hints:
   * Output of 1st step is file called `frameno.avi' with encoded audio

   * 2nd step is using `frameno.avi' and output is text file called
     `lavc_stats.txt' with timing informations

   * 3rd step is using `frameno.avi' and `lavc_stats.txt' for encoding
     the stream to the output file `movie2.avi'

   * If you want change only video bitrate, keep the file `frameno.avi'
     comment out the 1st step encoding and repeate 2nd and 3rd step.
     Dont forget to remove the line where the `frameno.avi' is removed.


File: mjpeg-howto.info,  Node: Optimizing the stream,  Next: Transcoding of existing MPEG-2,  Prev: Converting the stream to MPEG or DIVx videos,  Up: Top

8 Optimizing the stream
***********************

Using filters helps to increase the image quality of constant bitrate
(CBR) video streams. With VBR (variable bit rate) video the filesize is
reduced.

   Example:

   `> lav2yuv stream.avi | yuvmedianfilter | mpeg2enc -o video.m1v'

   Here the yuvmedianfilter program is used to improve the image. This
removes some of low frequence noise in the images. It also softens the
image a little. It takes a center pointer and averages the pixels
around it that fall within the specified threshold. It then replaces
the center pixel with this new value.  You can also use the -r (radius)
option for an other search radius.

   `NOTE:'a radius greater than the default value of 2 is horrendously
slow!

   yuvmedianfilter has separate settings for luma and chroma. You can
control the search radius and the trigger threshold independently.  If
you use a threshold of 0 then filtering is disabled (-t 0 disables luma
filtering, -T 0 disables chroma filtering).

   `> lav2yuv stream.avi | yuvmedianfilter -r 3 -t 4 -T 0 | mpeg2enc -o
video.m1v'

   This example uses a search radius of 3 pixels for the luma, a
threshold of 4 (the default is 2), and disables filtering for the
chroma components.   Sometimes, depending on the source material,
median filtering of the chroma can cause a slight color shift towards
green.   Filtering on the luma component (disabling the chroma
filtering) is the solution to that problem.

   Example:

   `> lav2yuv stream.avi | yuvdenoise | mpeg2enc -o video.m1v'

   Now we are using yuvdenoise to improve the image. The filter mainly
reduces color and luminance-noise and flickering due to phase errors
but is also effective at removing speckles.

   yuvdenoise denoises interlaced if the input is interlaced.  You can
of course change the denoiser threshold (-g/t).  Creating a black
border can lower the bitrate of the encoded stream because pure black
areas compress much better than noise (captures from analog sources
such as VHS and 8mm usually have several lines at the time and bottom
that are very noisy). For this you can use the scaler

   yuvdenoise uses a different approach to filter the noise.  More
information about how yuvdenoise works as well as descriptions of its
options are found in the manpage.

   If you have a high quality source you should lower the filter to
levels like that: -g 0,255,255 -t 2,2,2.  You might also use the
mpeg2enc `-h/-keep-hf' option. That option tells mpeg2enc to keep as
much high frequency information as possible.   Using -h will greatly
increase the bitrate (filesize).  If the bitrate is too close to the
maximum (set with -b) the encoder will have to decrease the quality to
avoid exceeding the maximum bitrate.

   A builtin filter in mpeg2enc is the -N/-reduce-HF option.  This
option is not really filter in the usual sense.  Rather it changes how
exactly the high frequency information is encoded.  Often the high
frequency is noise.  You also have high frequencies on sharp borders or
transitions. The -N option can have values between 0.0 and 2.0 where 0.0
does nothing (disables the high frequency quantizer boost) and 2.0 gives
the maximum quantization boost.  The value to use depends on the desired
output quality and filesize.  Values of -N less than 0.5 are very subtle
while a value of 1.0 will achieve a good balance between bitrate
reduction and output quality.   Using -N values above 1.5 will
noticeably reduce the sharpness of the output picture and are normally
used only for poor quality sources (VHS tapes for example).

   Using yuvmedianfilter's capability to only filter the chroma (-T) is
moderately effective at reducing noise in dark scenes without softening
the image during normal (brighter) scenes.   Median filtering of the
luma (-t) will produce a lower bitrate but can cause loss of detail
(softening).  Chroma only medianfiltering is less agressive and is a
good choice to use in combination with yuvdenoise.

   Combining the filters yuvdenoise, yuvmedianfilter and the mpeg2enc -N
option gives a very fine degree of control over the bitrate (filesize).
The reduction (or increase) in the bitrate depends on the source
material and the exact encoding/filter options used.  So we can give no
exact numbers how much each option and combination will reduce the
filesize, only guidelines.

   Usually you should use the -N option in a range from 0.5 to 1.5.
Below 0.5 it does not reduce the bitrate very much (but does preserve
sharpness).  At 1.5 and higher you will notice a softening in the video
and possibly artifacts (halo/ringing) around edges of objects
(text/subtitles especially).  If you combine the filters you should use
yuvdenoise and maybe afterwards yuvmedianfilter.  Maybe yuvmedianfilter
even after scaling.  Having yuvmedianfilter in the chain does not
reduce the bitrate that much.  Often the use of yuvdenoise is enough.
The yuvmedianfilter helps much if you have low quality sources, and not
that much if you already have a rather good quality.  When you combine
the filter and option you will very likely reduce the filesize to about
the half of the filesize without using the options and programs.

   In general aggressive filtering will produce smaller files (lower
bitrate) but reduce the quality (details) of the picture.  Less
aggressive filtering/processing will preserve more detail but result in
larger files.

   Example:

   `> lav2yuv stream.avi | yuvkineco -F 1 | mpeg2enc -o video.m1v'

   yuvkineco is used for NTSC sources. It does the conversation from
30000.0/1001.0 (about 29.97) fps to 24000.0/1001.0 (about 23.976) fps,
you can call it "reverse 2-3 pulldown" more info about this in the
README.2-3pulldown. yuvkineco does only remove NTSC specific problems.

   If you want to improve the image you should also use yuvdenoise:

   `> lav2yuv stream.avi | yuvkineco | yuvdenoise | mpeg2enc -o
video.m1v'

   Example

   `> lav2yuv stream.avi | yuvycsnoise | mpeg2enc -o video.m1v'

   yuvycsnoise is also used for NTSC and is specialized for NTSC Y/C
separation noise. If video capture hardware has only a poor Y/C
separator then at vertical stripes (especially red/blue) noises appear
which seem checker flag and bright/dark invert per 1 frame.
yuvycsnoise reduces noises of this type. You can also use different
thresholds for luma/chroma and the optimizing method.  This filter is
not needed with working with DV (Digital Video) data.

   yuvycsnoise works only correct when we have NTSC with:

   * full height (480 lines)

   * full motion captured (29.97 fps)

   * captured with poor Y/C separator hardware

   For more information about the yuvkineco and yuvycsnoise read the
README in the yuvfilters directory.

   If you want to experiment to determine the optimal settings for the
denoiser, scaler and so on replace the mpeg2enc with yuvplay.  yuvplay
plays back the yuv frames so you can see if the options you have chosen
are making the thing better or worse.

   A command would look like this:

   `> lav2yuv stream.eli | yuvdenoise -options | yuvscaler -options |
yuvplay'

   If you want to know how much each tool lowers the average bitrate.
You can use this table to see what you can expect if you have a full
size video and want to create a DVD with a qality factor of 5 and the
allowed maximal bitrate of 8500kb/sec.

   * no denoising : 8300 kb/s (mostly hitting the upper bound)

   * yuvenoise : 7700 kb/s

   * mpeg2enc -reduce-hf : 7400 kb/s

   * yuvdenoise + yuvmedianfilter : 6000 kb/s

   * yuvdenoise + mpeg2enc -reduce-hf : 4900 kb/s

   * all of the above : 3600 kb/s

   While `-N|-reduce-hf' or yuvdenoise alone is only a modest
improvement, together they reduce the bitrate substantially.  There is
not really much visible difference between using yuvdenoise alone and
yuvdenoise with mpeg2enc -reduce-hf. The usefull values are between 0.0
and 1.5. Where you can say that the higher the quality factor you want,
the less this option improves. At a quality factor 4 you save using -N
1.0 about 1%. If you want a quality factor of 9 and use the -N 1.0 you
might save up to 40%. But you might save less, that depends on the
video you encode!!!

   If you ask yourself why not alyways use all of the above filters?
Hmmm, hard question. The image softens, and the encoding time increases.
Each filter needs about the same amount of time as mpeg2enc needs for
encoding the video.

   If you have very high quality material and want to keep every detail
you should try to use the mpeg2enc -keep-hf|-h on the other hand

   `Note:' The bitrate reduction you have depends on the material and
on the noise of the images.

   A other interresting mpeg2enc option is the `-E|-unit-coeff-elim'
option. This option is disabled by default. If you enable it, a special
"unit coefficient elimination" algorithm, is applied to the encoded
picture blocks.   Basically this proceedure forces blocks of a type
that do not carry much information (but use many bits to encode) to be
skipped. A negative value examines the base (DC) as well as the AC
coefficients. A positive value means that only texture (AC)
coefficients are examined and possibly zeroed.  The recommended values
lies between -20 and +20. You usually can expect that you have a 5%
decreased filesize. The amount the bitrate is reduced can vary
considerably, the range spans from not really noticable up to 20%.

   If you think a other quantization matrice will help use the
`-K|-custom-quant-matrices' option. You can try out your own
quanitsation matrice or use another builtin than the default.  You can
choose between kvcd, tmpgenc, hi-res, and your own. Using -K usually
makes the file smaller except the hi-res option (that makes files
considerably larger). Exact guidelines are hard to give, sometime a
other quanitsation matrix saves almost nothing, and the next time up to
20%. More than 20% is very unlikely, 10-15% at a moderate qualityfactor
(-q 8-10) are likely.  The higher the qualiy the less it saves, at a
quality factor of 4-6 the reduction in bitrate may only be 5%

   One thing to keep in mind is that the unit coefficient elimination
and the quantization matrix option are decreasing the bitrate while
maintaining the same visual quality.   At this point you can chose to
use the smaller file to increase the amount of video that will fit on
the disc media or you could chose to increase the quality even more by
lowering the -q value by 1 and make a larger (but higher quality) file.

* Menu:

* Scaling and offset correction::
* Frame rate conversion::


File: mjpeg-howto.info,  Node: Scaling and offset correction,  Next: Frame rate conversion,  Up: Optimizing the stream

8.1 Scaling and offset correction
=================================

The basic scaling is described in the `Converting video' section

   The scaling, takes a part of the picture, and scales it to a larger
or smaler size. The scaling is done by yuvscaler:

   `lav2yuv test.eli | yuvscaler -I USE_400x400+50+100 | yuvplay'

   Here we only take part of the picture and scale it up to the size of
the original frame.  But yuvscaler also changes the pixel aspect ratio.
That means when you look at the stream using yuvplay it looks like a
square in our example.  After scaling, if the sample (pixel) aspect
ratio were not changed, the video would not display with the proper
aspect ratio.  Yuvscaler compensates by adjusting the sample aspect
ratio.  If you have a interlaced video, the height and HeightOffset
have to be a multiple by 4 if the video is interlaced. Else the values
(width, height, widthoffset, heightoffset) have to be a multiple of 2.

   A problem that cannot be solved easily with scaling is when the
picture is not centered horizontal. On one side you have no black
pixels and on the other you have 30 for example. Scaling is here is the
wrong solution.  y4mshift is the perfect solution because it can shift
the image to the left or right.

   `lav2yuv test.eli | y4mshift -n 20 | mpeg2enc -f 3 -b 4000 -q 10 -o
video.m2v'

   That will shift the image 20 pixels to the right. If you use a
negative the image is shift to the left. You have to use a even number.
The inserted pixels are set to black.

   Some might wonder why the image is not centered and there is a black
border around the image when you view what you have recorded. The
reason for the black border is the TV (CRT = Catode Ray Tube) and a
really interresting storry about how the TV standart was definden. But
tha topic is described in other books.

   The TV does not show the full picture. A part of the picture is not
shown because the TV sets overscan (sometimes as much as 10% but more
common today is 5%).  But when you capture the video with a card you
see the whole image including the border that TVs lose due to
overscanning.  A horizontal offset is usually not a problem of the
capture card. It is a problem when the film is broadcast and not well
synchronized with the image.  This means that the scan of the source
not exactly synchronized with the carrier signal, you wont see that on
TV.


File: mjpeg-howto.info,  Node: Frame rate conversion,  Prev: Scaling and offset correction,  Up: Optimizing the stream

8.2 Frame rate conversion
=========================

Ever needed to convert the framerate from PAL to NTSC or the other
direction around ? Or something much simpler like converting the
framerate from 24FPS to 24000:1001 for conversation from a film frame
rate to a valid NTSC frame rate.

   Than `yuvfps' is your program. It can lower the framerate by dropping
frames, or create a higher framerate by replicating frames. If you have
a wrong framerate in the header you can only change the header of the
YUV stream and not modify the stream.

   Because the frames are only replicated (copied) you should denoise
first and then change the framerate and scale at als last step. If you
have a interlaced source you should also deinterlace before changeing
the framerate. If you create a higher frame rate it is very likely that
you will have weird flickers when you play it back. If you convert PAL
to NTSC (30000:1001 FPS about 29,97 FPS) the frame rate will lower by
about the factor 480/576 (NTSC lines / PAL lines).  If you lower the
frame rate from PAL to NTSC (at 24000:1001) or NTSC FILM (24FPS) the
bitrate will be about (480 Lines * 24 FPS) / (576 Lines * 25FPS).  If
you change the frame rate before denoising the yuvdenoise will have
problems finding the noise across the frames, so the needed bandwith
will slightly increase.

   Example

   `> lav2yuv video.eli | yuvfps -r 30000:1001 | yuvscaler -O SVCD |
mpeg2enc -f 4 -o video_ntsc_svcd.m2v'

   This is a example to convert the source video to a NTSC video
running at 30000:1001 FPS (or about 29,97FPS) at SVCD size.

   Example

   `> lav2yuv video.eli | yuvdenoise | yuvfps -r 24000:1001 | yuvscaler
-O SIZE_720x480 | mpeg2enc -f 3 -b 4000 -q 7 -o video_ntsc.m2v'

   This example shows how you should use the tools. Denoise first and
than change the framerate and in the last step change the image size.

   It can happen that yuvscaler or mpeg2enc do not detect the TV norm
correct. If that happens you have to add the norm option `-n n/p/s' to
the program that chooses the wrong norm.

   If you know that the header tells the wrong framerate, you can
simply change the framerate of the yuv header this way:

   `> lav2yuv video.eli | yuvfps -r 25:1 -c | mpeg2enc -f 3 -b 4000 -q
7 -o video_pal.m2v'

   You need the `-c' option. To tell yuvfps that it only should change
the header of the stream. With the `-r 25:1' you tell yuvfps the frame
rate it should write into the header. In your example the PAL frame
rate of 25 FPS. You always have to use the fractional form.

   If you know that the header is wrong, and you need a different output
bitrate you can do this in a single step:

   `> lav2yuv video.eli | yuvfps -s 24:1 -r 25:1 | mpeg2enc -o
video.m1v'


File: mjpeg-howto.info,  Node: Transcoding of existing MPEG-2,  Next: Trading Quality/Speed,  Prev: Optimizing the stream,  Up: Top

9 Transcoding of existing MPEG-2
********************************

For transcoding existing MPEG-2 streams from digital TV cards or DVD a
lower data-rate than for broadcast will give good results.  Standard
VCD 1152 kbps typically works just fine for MPEG1. The difference is in
the Signal/Noise ratio of the original. The noise in the analog stuff
makes it much harder to compress.

   One other very good guide that helps you transcoding videos can be
found at: http://www.bunkus.org/dvdripping4linux/index.html

   You will also need to manually adjust the audio delay offset
relative to video when multiplexing. Very often around 150ms delay
seems to do the trick.

   You have to download the ac3dec and mpeg2dec packages. You can find
them at mjpeg homepage ( http://sourceforge.net/projects/mjpeg ).  You
also need sox and toolame.

   In the scripts directory there is a `mpegtranscode' script that does
most of the work.

   So transcoding looks like this:

   `> mjpegtranscode -V -o vcd_stream mpeg2src.mpg'

`-V'
     set's the options so that a VCD compatible stream is generated

`-o vcd_stream'
     a vcd_stream.m1v (video) and vcd_stream.mp2 (audio) is created

`mpeg2src.mpg'
     specifies the source stream


   The script prints also something like this:

   `> SYNC 234 mSec'

   You will need to adjust the audio/video startup delays when
multiplexing to ensure audio and video are synchronized.  The exact
delay (in milliseconds) that you need to pass to mplex to synchronize
audio and video using the "-v"" is printed by the extract_a52 tool
labeled "SYNC" when run with the "s" flag. This is the value th
mjpegtranscode script prints out after the `SYNC' word.

   Then you need to multiplex them like this:

   `> mplex -f 1 -O 234 vcd_stream.mp2 vcd_stream.m1v -o lowrate.mpg'

`-f 1'
     Mux format is set to VCD

`-O 234'
     Video timestamp offset in mSec, generated by the mjpegtranscoding
     script, there negative values are allowed

`vcd_stream.mp2 & vcd_stream.m1v'
     generated files by the script

`lowrate.mpg'
     the VCD compatible output stream


   Here we have a SVCD (MPEG-2 video) example:

   `> mjpegtranscode -S -o svcd_stream mpeg2src.mpg'

   You have to multiplex it with:

   `> mplex -f 4 -O 234 svcd_stream.mp2 svcd_stream.m2v -o lowrate.mpg'

   `Problem:' There is sometimes a problem with NTSC and VCD playback
because movies may be recoded with 3:2 pulldown NTSC with 60
fields/sec. mpeg2dec is designed for playback on computers and
generates the original 24frames/sec bitrate. If you encode the video
now 30frames/sec video is created. This video is now much too short for
the encoded audio.

   The transcoding can be made to work but it must be done manually:

   `> mpeg2dec -s -o pgmpipe mpeg2src.mpg | pgmtoy4m -a 59:54 -r 25:1
-i t | mpeg2enc -I 0 -f 4 -q 9 -V 230 -p -P -o svcd_stream.m2v'

   The -p tells mpeg2enc to generate header flags for 3:2 pull down of
24fps movie. It may also work if you do not add the -p flag.  You do
not need the -p flag when transcoding to VCD format because it is not
supported in mpeg1.

* Menu:

* If you want to do every step on your own it will look something like this::


File: mjpeg-howto.info,  Node: If you want to do every step on your own it will look something like this,  Up: Transcoding of existing MPEG-2

9.1 If you want to do every step on your own it will look something like this
=============================================================================

Extracting Audio:

   `> cat test2.mpg | extract_a52 - -s | ac3dec -o wav -p sound.wav
2>/dev/null'

   One of the first lines showed contains the label "SYNC" you have to
use this time later when multiplexing. The 2>/dev/null redirects the
output of ac3dec to /dev/null.  In the next step you generate the mpeg
audio file:

   `> cat sound.wav | mp2enc -V -v 2 -o audio.mp2'

`-V'
     forces VCD format, the sampling rate is converted to 44.1kHz from
     48kHz

`-v 2'
     unnecessary but if you use it mp2enc tells you how many seconds of
     the audio file are already encoded.

`-o'
     Specifies the output file.


   `cat test2.mpg | extract_a52 - -s | ac3dec -o wav | sox -t wav
/dev/stdin -t wav -r 44100 /dev/stdout | toolame -p 2 -b 224 /dev/stdin
audio.mp2'

   One of the first lines again output contains the label "SYNC".  You
have to use this time (referred to as "SYNC_value" below) when doing the
multiplexing.

   For VCD creation use:

   `> mpeg2dec -s -o pgmpipe test2.mpg | pgmtoy4m -a 59:54 -r 25:1 -i t
| mpeg2enc -s -o video_vcd.m1v'

`'
     mpeg2dec:

`-s'
     tells mpeg2dec to use program stream demultiplexer

`-o pgmpipe'
     the output format of the pictures, suitable for pgmtoy4m


   Mplex with:

   `> mplex -f 1 -O SYNC_value audio.mp2 video_vcd.m1v -o
vcd_stream.mpg'

`-f 1'
     generates an VCD stream

`-O SYNC_value'
     the value mentioned above


   For SVCD creation use:

   `> mpeg2dec -s -o mpeg2src.mpg | pgmtoy4m -a 59:54 -r 25:1 -i t  |
mpeg2enc -f 4 -q 9 -V 230 -o video_svcd.mpg'

`-q 9'
     Quality factor for the stream (VBR stream) (default q: 12)

`-V 230'
     Target video buffer size in KB

`-o'
     Output file


   Mplex with:

   `> mplex -f 4 -b 230 audio.mp2 video_svcd -o svcd_stream.mpg'

`-f 4'
     generate an SVCD stream

`-b 200'
     Specify the video buffer size by the playback device.


   For other video output formats this might work:

   `> mpeg2dec -s -o pgmpipe test2.mpg | pgmtoy4m -a 59:54 -r 25:1 -i t
| yuvscaler -O SIZE_320x200 -O NOT_INTERLACED | mpeg2enc -o
strange_video.m1v'

   If you want to edit mpeg streams, this also works, but in a slightly
different way. For demultiplexing you can use bbdmux, from the bbtools
package. Splits out either video or audio very cleanly.  You can't get
it any more from the homepage from Brent Beyler, it can still be found
when you search for it using that keywords " bbtools linux -suse
-blackbox". Currenty it can be found at: http://www.nop.org/inkling/

   First run:

   `> bbdmux myvideo.mpg'

   You should get something like this:

   Found stream id 0xE0 = Video Stream 0 Found stream id 0xC0 = MPEG
Audio Stream 0 Found stream id 0xBE = Padding Stream

   Extract audio with:

   `> bbdmux myvideo.mpg 0xC0 audio.mp1'

   Convert it to wav:

   `> mpg123 -w audio.wav audio.m1v'

   Extract video with:

   `> bbdmux myvideo.mpg 0xE0 video.m1v'

   Converting video to an mjpeg avi stream:

   `> mpeg2dec -o pgmpipe video.m1v | pgmtoy4m -a 59:54 -r 25:1 -i t |
yuv2lav -f a -o test.avi'

   Then adding the sound to the avi:

   `> lavaddwav test.avi audio.wav final.avi'

   If the source video has already the size of the target video use -o
YUV. Using YUVh makes the video the half size!  The rest can be done
just like editing and encoding other streams.  If you have videos with
ac3 sound you only have to adapt the commands above.

   Extracting Audio:

   `> cat test2.mpg | extract_a52 - -s | ac3dec -o wav 2>dev/null
>sound.wav'

   Extract video and adding the audio in a single step :

   `> mpeg2dec -s -o pgmpipe | pgmtoy4m -a 59:54 -r 25:1 -i t |
yuvscaler -O VCD | yuv2lav -f a -q 85 -w sound.wav -o test.avi'

   `NOTE:'You need much disk space. 1GB of video has a size of about 2GB
at SVCD format and of course disk space is needed for some temp files.
Converting the video to mjpeg also takes some time.  On my Athlon 500 I
never get more than 6-7 Frames a second.  You loose quality each time
you convert a stream into an other format!


File: mjpeg-howto.info,  Node: Trading Quality/Speed,  Next: SMP and distributed Encoding,  Prev: Transcoding of existing MPEG-2,  Up: Top

10 Trading Quality/Speed
************************

If absolute quality is your objective a modest improvement can be
achieved using the -4 and -2 flags.  These control how ruthlessly
mpeg2enc discards bad looking matches between sections of adjacent
frames during the early stages of the search when it is working with
4*4 and 2*2 clusters of pixels rather than individual pixels. Setting
-4 1 -2 1 maximizes quality. -4 4 -2 4 maximizes speed. Note that
because the statistical criteria mpeg2enc uses for discarding bad
looking matches are usually fairly reliable the increase/decrease in
quality is modest (but noticeable).

   Reducing the radius of the search for matching sections of images
also increases speed. However due to the way the search algorithm works
the search radius is in effect rounded to the nearest multiple of 8.
Furthermore, on modern CPU's the speed gained by reducing the radius
below 16 is not large enough to make the marked quality reduction
worthwhile for most applications.

* Menu:

* Creating streams to be played from disk using Software players::


File: mjpeg-howto.info,  Node: Creating streams to be played from disk using Software players,  Up: Trading Quality/Speed

10.1 Creating streams to be played from disk using Software players
===================================================================

Usually MPEG player software is much more flexible than the hardware
built into DVD and VCD players. This flexibility allows for
significantly better compression to be achieved for the same quality.
The trick is to generate video streams that use big video buffers
(500KB or more) and variable bitrate encoding (the -f, -q flag to
mpeg2enc). Software players will often also correctly play back the
more efficient MPEG layer 3 (yes, "MP3" audio format.  A good MP3
encoder like lame will produce results comparable to layer 2 at 224Kbps
at 128Kbps or 160Kbps.


File: mjpeg-howto.info,  Node: SMP and distributed Encoding,  Next: Interoperability,  Prev: Trading Quality/Speed,  Up: Top

11 SMP and distributed Encoding
*******************************

The degree to which mpeg2enc tries to split work between concurrently
executing threads is controlled by the -M or -multi-thread [0..32]
option. This optimizes mpeg2enc for the specified number of CPUs. By
default (-M 1), mpeg2enc runs with just a little multi-threading:
reading of frames happens concurrently with compression. This is done
to allow encoding pipelines that are split across several machines (see
below) to work efficiently without the need for special buffering
programs.  If you are encoding on a single-CPU machine where RAM is
tight you may find turning off multithreading altogether by setting -M
0 works slightly more efficiently.

   For SMP machines with two ore more processors you can speed up
mpeg2enc by setting the number of concurrently executing encoding
threads's you wish to utilize (e.g. -M 2). Setting -M 2 or -M 3 on a
2-way machine should allow you to speed up encoding by around 80%.
Values above 3 are accepted but have very little effect even on 4 cpu
systems.

   If you have a real fast SMP machine (currently 1.Aug.03) like a dual
Athlon MP 2600 or something similar the -M 2 and the filtering might not
keep both (or more)  CPU's busy. The use of the buffer or bfr program
with a 10-20MB buffer helps to keep both CPUs busy.

   Obviously if your encoding pipeline contains several filtering stages
it is likely that you can keep two or more CPU's busy simultaneously
even without using -M. Denoising using yuvdenoise or yuvmedianfilter is
particular demanding and uses almost as much processing power as MPEG
encoding.

   It you more than one computer you can also split the encoding
pipeline between computers using the standard 'rsh' or 'rcmd' remote
shell execution commands. For example, if you have two computers:

   `> rsh machine1 lav2yuv "mycapture.eli | yuvscaler -O SVCD |
yuvdenoise" | mpeg2enc -f 4 -o mycapture.m2vi'

   Here the computer where you execute the command is doing the MPEG
encoding and "machine1" is the machine that is decoding scaling and
denoising the captured video.

   Obviously, for this to work "machine1" has to be able to access the
video and the computer where the command is executed has to have space
for the encoded video. In practice, it is usually well worth setting up
network file-storage using "NFS" or other packages if you are going to
do stuff like this.  If you have three computers you can take this a
stage further, one computer could do the decoding and scaling, the next
could do denoising and the third could do MPEG encoding:

   `> rsh machine1 "lav2yuv mycapture.eli | yuvscaler -O SVCD" |
yuvdenoise | rsh machine3 mpeg2enc -f 4 -o mycapture.m2v'

   `NOTE:'How the remote command executions are set up so that the data
is sent direct from the machine that produces it to the machine that
consumes it.

   In practice for this to be worthwhile the network you are using must
be fast enough to avoid becoming a bottleneck. For Pentium-III class
machines or above you will need a 100Mbps Ethernet.

   For really fast machines a switched 100MBps Ethernet (or better!) may
be needed.Setting up the rshd ("Remote Shell Daemon" needed for rsh to
do its work and configuring "rsh" is beyond the scope of this document,
but its a standard package and should be easily installed and activated
on any Linux or BSD distribution.

   Be aware that this is potentially a security issue so use with care
on machines that are visible to outside networks!


File: mjpeg-howto.info,  Node: Interoperability,  Prev: SMP and distributed Encoding,  Up: Top

12 Interoperability
*******************

Quicktime files capturing using lavrec can be edited using
Broadcast2000.  But Broadcast2000 is not available any more on
heroinewarrior.  mjpeg AVI files captured using the streamer tool from
the xawtv package can be edited and compressed and played back using
software.  Hardware playback is not possible for such files due to
limitations in the Zoran hardware currently supported. Videos recorded
with NuppelVideo can also be processed with the mjpeg tools.

   If you have a Macintosh (MAC) and want to use the mjpeg tools look
there: http://www.sjoki.uta.fi/~shmhav/SVCD_on_a_Macintosh.html

   If you want to compile the mjpeg-tools on your MAC, our just want
mpeg2enc and mplex compiled for the MAC take a look here:
http://mjpeg.sf.net/MacOS/

   MPEG files produced using the tools are know to play back correctly
on:

   * dxr2 (hardware decoder card)

   * xine http://xine.sourceforge.net/

   * dvdview http://rachmaninoff.informatik.uni-mannheim.de/dvdview/

   * xmovie http://heroinewarrior.com/xmovie.php3

   * mplayer http://www.mplayerihq.hu/

   * vlc http://www.videolan.org/

   * MPEG1 only: gtv
     http://packages.debian.org/stable/graphics/smpeg-gtv

   * MS Media player version 6 and 7

   * SW DVD Player

   To find out what you HW-player (most of the time DVD player) can do
take a look at: http://www.videohelp.com

   It seems that the MS Media player likes MPEG-1 streams more if you
have used -f 1 when multiplexing.

   If you have any problems or suggestions feel free to mail me
(Bernhard Praschinger): waldviertler@users.sourceforge.net There is a
lot of stuff added from the HINTS which Andrew Stevens created.
Wolfgang Goeller and Steven M. Schultz checked the document for bugs
and spelling mistakes.

   And to the people who have helped me with program descriptions and
hints, `thanks'



Tag Table:
Node: Top133
Node: Introduction784
Node: Unsorted list of useful Hints2475
Node: Some books we found usefull7024
Node: Recording videos7733
Node: lavrec examples8117
Node: Other recording hints11900
Node: Some information about the typical lavrec output while recording13432
Node: Notes about "interlace field order - what can go wrong and how to fix it"14987
Node: There are three bad things that can happen with fields15832
Node: How can I recognize if I have one of these Problems ?17617
Node: How can you fix it?19234
Node: Hey what about NTSC movies ?22539
Node: Creating videos from other sources23862
Node: Creating videos from images24447
Node: Decoding streams with mplayer27623
Node: Decoding MPEG2 streams with mpeg2dec28999
Node: Other things to know30053
Node: Checking if recording was successful30651
Node: Edit the video32915
Node: Edit with glav33223
Node: Unify videos34671
Node: Separate sound35161
Node: Separate images35588
Node: Creating movie transitions36583
Node: Converting the stream to MPEG or DIVx videos40304
Node: Creating sound42044
Node: Converting video43847
Node: Scaling45574
Node: Putting the streams together47846
Node: Creating MPEG1 Videos50139
Node: MPEG1 Audio creation Example51036
Node: MPEG1 Video creation Example51843
Node: MPEG1 Multiplexing Example56386
Node: Creating MPEG2 Videos57259
Node: MPEG2 Audio creation Example58314
Node: MPEG2 Video creation Example58921
Node: Which values should be used for VBR Encoding61362
Node: Encoding destination TV (interlaced) or Monitor (progressive)63679
Node: MPEG2 Multiplexing Example66235
Node: Creating Video-CD's67053
Node: VCD Audio creation Example68127
Node: VCD Video creation Example68686
Node: VCD Multiplexing Example70212
Node: Creating the CD70578
Node: Notes71139
Node: Storing MPEGs72142
Node: Creating SVCD73485
Node: SVCD Audio creation Example74298
Node: SVCD Video creation Example75280
Node: SVCD Multiplexing Example77707
Node: SVCD Creating the CD78254
Node: Creating DVD's78942
Node: DVD Audio creation Example79899
Node: DVD Video creation Example80456
Node: DVD Multiplexing Example81441
Node: DVD creation Example81960
Node: Creating DIVX Videos82984
Node: lav2avi-sh83189
Node: Optimizing the stream85797
Node: Scaling and offset correction96522
Node: Frame rate conversion99036
Node: Transcoding of existing MPEG-2101891
Node: If you want to do every step on your own it will look something like this105211
Node: Trading Quality/Speed109520
Node: Creating streams to be played from disk using Software players110746
Node: SMP and distributed Encoding111569
Node: Interoperability115211

End Tag Table
